# Overview

## Introduction

This API document mainly defines the development interface of the Anviz SDK, which provides reference for developers to connect and operate related devices.

This document is mainly related to the software development engineers, software testing engineers and project managers.

## Overview of functions

This API document mainly provides some interfaces of the client/server to the PC end, getting the parameters of the time attendance/access control, and setting the configuration and parameters of the time attendance/access control device. In order to support multiple devices, the interfaces between queries and settings exist asynchronously. SDK is compiled into the form of a dynamic library.

## System logic structure

Device

PC

CChex\_Init

CChex\_Start

CChex\_Stop

Start

CChex\_GetNetConfig

CChex\_SetNetConfig

CChex\_Update

SDK

SetNetwork

GetNetwork

Result

Stop

## Brief introduction of interface functions

uint CChex\_Version();

void CChex\_Init();

IntPtr CChex\_Start();

void CChex\_Stop(IntPtr CchexHandle);

int CChex\_Update(IntPtr CchexHandle, int[] DevIdx, int[] Type, IntPtr Buff, int Len);

int CChex\_GetNetConfig(IntPtr CchexHandle, int DevIdx);

int CChex\_SetNetConfig(IntPtr CchexHandle, int DevIdx, ref CCHEX\_NETCFG\_INFO\_STRU Config);

int CChex\_MsgGetByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

int CChex\_MsgDelByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

int CChex\_MsgAddNew(IntPtr CchexHandle, int DevIdx, byte[] Data, int Len);

int CChex\_MsgGetAllHead(IntPtr CchexHandle, int DevIdx);

int CChex\_RebootDevice(IntPtr CchexHandle, int DevIdx);

int CChex\_SetTime(IntPtr CchexHandle, int DevIdx, int Year, int Month, int Day, int Hour, int Min, int Sec);

int CChex\_GetSNConfig(IntPtr CchexHandle, int DevIdx);

int CChex\_DownloadAllRecords(IntPtr CchexHandle, int DevIdx);

int CChex\_DeleteRecordInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_RECORD\_INFO\_STRU Config);

int CChex\_GetBasicConfigInfo(IntPtr CchexHandle, int DevIdx);

int CChex\_SetBasicConfigInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_BASIC\_CFG\_INFO\_STRU Config);

int CChex\_ListPersonInfo(IntPtr CchexHandle, int DevIdx);

int CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_PERSON\_INFO\_STRU Config);

int CChex\_DownloadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

int CChex\_UploadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

int CChex\_GetTime(IntPtr CchexHandle, int DevIdx);//(24)

int CChex\_InitUserArea(IntPtr CchexHandle, int DevIdx);

int CChex\_InitSystem(IntPtr CchexHandle, int DevIdx);

int CChex\_GetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx);

int CChex\_SetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF config);

int CChex\_GetPeriodTime(IntPtr CchexHandle, int DevIdx, byte SerialNumbe);

int CChex\_SetPeriodTime(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_PERIOD\_TIME\_STRU\_EXT\_INF config);

int CChex\_GetTeamInfo(IntPtr CchexHandle, int DevIdx, byte TeamNumbe);

int CChex\_SetTeamInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_TEAM\_INFO\_STRU\_EXT\_INF config);

int CCHex\_AddFingerprintOnline(IntPtr CchexHandle, int DevIdx, ref CCHEX\_ADD\_FINGERPRINT\_ONLINE\_STRU\_EXT\_INF Param);

int CCHex\_ForcedUnlock(IntPtr CchexHandle, int DevIdx, ref CCHEX\_FORCED\_UNLOCK\_STRU\_EXT\_INF Param);

int CCHex\_Udp\_Search\_Dev(IntPtr CchexHandle);

int CCHex\_Udp\_Set\_Dev\_Config(IntPtr CchexHandle, ref CCHEX\_UDP\_SET\_DEV\_CONFIG\_STRU\_EXT\_INF config);

int CCHex\_ClientConnect(IntPtr CchexHandle, byte[] Ip, int Port);

int CCHex\_ClientDisconnect(IntPtr CchexHandle, int DevIdx);

## Message Type

CChex\_Update(anviz\_handle, dev\_idx, Type, pBuff, len);

You need to loop the query to see if there is an asynchronous return, and if you have a different Type of data parsing, get the data you want.public enum MsgType:int

{

CCHEX\_RET\_RECORD\_INFO\_TYPE = 1

, CCHEX\_RET\_DEV\_LOGIN\_TYPE

, CCHEX\_RET\_DEV\_LOGOUT\_TYPE

, CCHEX\_RET\_DLFINGERPRT\_TYPE = 4

, CCHEX\_RET\_ULFINGERPRT\_TYPE

, CCHEX\_RET\_MODIFY\_PERSON\_INFO\_TYPE = 8

, CCHEX\_RET\_LIST\_PERSON\_INFO\_TYPE

, CCHEX\_RET\_MSGGETBYIDX\_INFO\_TYPE = 12

, CCHEX\_RET\_MSGGETBYIDX\_UNICODE\_INFO\_TYPE

, CCHEX\_RET\_MSGADDNEW\_INFO\_TYPE

, CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

, CCHEX\_RET\_MSGDELBYIDX\_INFO\_TYPE // 15

, CCHEX\_RET\_MSGGETALLHEAD\_INFO\_TYPE

, CCHEX\_RET\_REBOOT\_TYPE

, CCHEX\_RET\_DEV\_STATUS\_TYPE

, CCHEX\_RET\_MSGGETALLHEADUNICODE\_INFO\_TYPE

, CCHEX\_RET\_SETTIME\_TYPE // 20

, CCHEX\_RET\_UPLOADFILE\_TYPE

, CCHEX\_RET\_GETNETCFG\_TYPE

, CCHEX\_RET\_SETNETCFG\_TYPE

, CCHEX\_RET\_GET\_SN\_TYPE //24

, CCHEX\_RET\_GET\_BASIC\_CFG\_TYPE = 29

, CCHEX\_RET\_SET\_BASIC\_CFG\_TYPE

, CCHEX\_RET\_DEL\_PERSON\_INFO\_TYPE = 31

, CCHEX\_RET\_DEL\_RECORD\_OR\_FLAG\_INFO\_TYPE = 33

,CCHEX\_RET\_GET\_BASIC\_CFG2\_TYPE = 37

,CCHEX\_RET\_SET\_BASIC\_CFG2\_TYPE = 38

,CCHEX\_RET\_GETTIME\_TYPE = 39

,CCHEX\_RET\_INIT\_USER\_AREA\_TYPE = 40

,CCHEX\_RET\_INIT\_SYSTEM\_TYPE = 41

,CCHEX\_RET\_GET\_PERIOD\_TIME\_TYPE = 42

,CCHEX\_RET\_SET\_PERIOD\_TIME\_TYPE = 43

,CCHEX\_RET\_GET\_TEAM\_INFO\_TYPE = 44

,CCHEX\_RET\_SET\_TEAM\_INFO\_TYPE = 45

,CCHEX\_RET\_ADD\_FINGERPRINT\_ONLINE\_TYPE = 46

,CCHEX\_RET\_FORCED\_UNLOCK\_TYPE = 47

,CCHEX\_RET\_UDP\_SEARCH\_DEV\_TYPE = 48

,CCHEX\_RET\_UDP\_SET\_DEV\_CONFIG\_TYPE = 49

,CCHEX\_RET\_GET\_INFOMATION\_CODE\_TYPE = 50

,CCHEX\_RET\_SET\_INFOMATION\_CODE\_TYPE = 51

,CCHEX\_RET\_GET\_BELL\_INFO\_TYPE = 52

,CCHEX\_RET\_SET\_BELL\_INFO\_TYPE = 53

,CCHEX\_RET\_LIVE\_SEND\_ATTENDANCE\_TYPE = 54

,CCHEX\_RET\_GET\_USER\_ATTENDANCE\_STATUS\_TYPE = 55

,CCHEX\_RET\_SET\_USER\_ATTENDANCE\_STATUS\_TYPE = 56

,CCHEX\_RET\_CLEAR\_ADMINISTRAT\_FLAG\_TYPE = 57

,CCHEX\_RET\_GET\_SPECIAL\_STATUS\_TYPE = 58

,CCHEX\_RET\_GET\_ADMIN\_CARD\_PWD\_TYPE = 59

,CCHEX\_RET\_SET\_ADMIN\_CARD\_PWD\_TYPE = 60

,CCHEX\_RET\_GET\_DST\_PARAM\_TYPE = 61

,CCHEX\_RET\_SET\_DST\_PARAM\_TYPE = 62

,CCHEX\_RET\_GET\_DEV\_EXT\_INFO\_TYPE = 63

,CCHEX\_RET\_SET\_DEV\_EXT\_INFO\_TYPE = 64

,CCHEX\_RET\_GET\_BASIC\_CFG3\_TYPE = 65

,CCHEX\_RET\_SET\_BASIC\_CFG3\_TYPE = 66

,CCHEX\_RET\_CONNECTION\_AUTHENTICATION\_TYPE = 67

,CCHEX\_RET\_GET\_RECORD\_NUMBER\_TYPE = 68

,CCHEX\_RET\_GET\_RECORD\_BY\_EMPLOYEE\_TIME\_TYPE = 69

,CCHEX\_RET\_GET\_RECORD\_INFO\_STATUS\_TYPE = 70

,CCHEX\_RET\_GET\_NEW\_RECORD\_INFO\_TYPE = 71

,CCHEX\_RET\_ULEMPLOYEE2W2\_INFO\_TYPE = 72,

CCHEX\_RET\_GET\_BASIC\_CFG5\_TYPE = 73,

CCHEX\_RET\_SET\_BASIC\_CFG5\_TYPE = 74,

CCHEX\_RET\_GET\_CARD\_ID\_TYPE = 75,

CCHEX\_RET\_SET\_DEV\_CURRENT\_STATUS\_TYPE = 76,

CCHEX\_RET\_GET\_URL\_TYPE = 77,

CCHEX\_RET\_SET\_URL\_TYPE = 78,

CCHEX\_RET\_GET\_STATUS\_SWITCH\_TYPE = 79,

CCHEX\_RET\_SET\_STATUS\_SWITCH\_TYPE = 80,

CCHEX\_RET\_GET\_STATUS\_SWITCH\_EXT\_TYPE = 81,

CCHEX\_RET\_SET\_STATUS\_SWITCH\_EXT\_TYPE = 82,

CCHEX\_RET\_UPDATEFILE\_STATUS\_TYPE = 83,

,CCHEX\_RET\_CLINECT\_CONNECT\_TYPE = 200

,CCHEX\_RET\_CLINECT\_DISCONNECT\_TYPE = 201

};

## Setup label and print setup Description

Generic version:

Default Setup: After download new records mark as:0(NO) Print LOG:0(NO)

W2 Version：

Default Setup: After download new records mark as:1(Yes) Print LOG:0(NO)

Customize(S) Version：

Default Setup: After download new records mark as:1(Yes) Print LOG:0(NO)

Customize（F）Version：：

Default Setup: After download new records mark as:0(NO) Print LOG:0(NO)

Change Configuration path:

1：Defining the configuration file：tc-b\_new\_sdk.ini

[LogFile]

LogFile = 1 1：yes 0：no

[SetRecordFlag]

SetRecordFlag = 1 1：yes 0：no

[Debug]

Debug = 0

2:Call the function interface：void CChex\_SetSdkConfig(void \*CchexHandle,int SetRecordflag,int SetLogFile);

Parameter：

int SetRecordflag 1：yes 0：no

int SetLogFile 1：yes 0：no

Priority level:

High： Call the function interface

High： Defining the configuration file

Low： Defining Setup

Notice：When without any “Call the function interface” and “Defining the configuration file as “Defining Setup”

# Description interface

## CChex\_Version

### Description functions

【Function】Query SDK Version.

### Request

【Mode】uint CChex\_Version()

【Parameter】None

### Response

【Return value】Get SDK version, Returns the version number of an integer number.

### Sample

int sdk\_ver = CChex\_Version();

### Notice

## CChex\_Init

### Description functions

【Function】 The SDK function initializes and initializes the socket application interface.

### Request

【Mode】void CChex\_Init()

【Parameter】None

### Response

【Return value】None

### Sample

CChex\_Init();

### Notice

None

## CChex\_Start

### Description functions

【Function】 Start the SDK, allocate space, and establish communication with the Anviz device.

### Request

【Mode】IntPtr CChex\_Start()

【Parameter】None

### Response

【Return value】Return the handle of SDK.

### Sample

IntPtr sdk\_handle = CChex\_Start();

if (sdk\_handle != null)

{

MessageBox.Show("Startup OK");

｝ else

{

MessageBox.Show("Startup errors,Please restart the program.");

}

### Notice

1. Make sure that CChex\_Init is initialized before run.

## CChex\_Stop

### Description functions

【Function】Stop the SDK, release the space, close the socket chain and so on.

### Request

【Mode】void CChex\_Stop(IntPtr CchexHandle)

【Parameter】CchexHandle,CChex\_Start successfully create the handle

### Response

【Return value】None

### Sample

CChex\_stop();

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_Update

### Description functions

【Function】The Return value get or set asynchronously.。

### Request

【Mode】int CChex\_Update(IntPtr CchexHandle, int[] DevIdx, int[] Type, IntPtr Buff, int Len);

【Parameter】CchexHandle,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx,Device index returned asynchronously,Output[Parameter]；

Buff,Returned data section,Output [Parameter]；

Len,Returns the length of the data section,Input[Parameter]；

### Response

【Return value】> 0：Successful asynchronous ; Return value == 0：Invalid Return value；< 0：buffer space is not enough，based on Return value, then re-apply the space.

### Sample

int ret = CChex\_Update(anviz\_handle, dev\_idx, Type, pBuff, len);

if (ret > 0)

{

switch(Type)

{

case CCHEX\_RET\_DEV\_LOGIN\_TYPE: // Connect the Anviz device successfully and return the Device ID, Device IP address, Software version, Device type and software version, etc.

break;

case CCHEX\_RET\_GET\_BASIC\_CFG\_TYPE: // Some basic information about the Anviz device, such as administrator password, firmware version, volume, etc.

break;

case CCHEX\_RET\_DEV\_STATUS\_TYPE: // Total number of employees, total number of fingerprints, total number of passwords, total number of cards, total attendance records, total new attendance record.

default:

break;

}

}else if (ret == 0)

{

// invalid data

}else

{

// Buff is not enough,

}

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetNetConfig

### Description functions

【Function】Query Anviz device’s network Configuration

### Request

【Mode】int CChex\_GetNetConfig(IntPtr CchexHandle, int DevIdx);

【Parameter】CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx,search the device Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GETNETCFG\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [4]IpAddr;// IP address

byte [4]IpMask;// Mask

byte [6]MacAddr;// MAC

byte [4]GwAddr;// Gateway

byte [4]ServAddr;// Sever IP address

byte RemoteEnable;//Standby

byte [2]Port;// Port

byte Mode;// Mode：0: Server，1:Client

byte DhcpEnable;// DHCP，0:Disable，1:Enable

### Sample

int ret = CChex\_GetNetConfig();

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetNetConfig

### Description functions

【Function】Set the network configuration of the Anviz device.

### Request

【Mode】int CChex\_SetNetConfig(IntPtr CchexHandle, int DevIdx, ref CCHEX\_NETCFG\_INFO\_STRU Config);

【Parameter】CchexHandle：,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config:

byte [4]IpAddr;// IP Address

byte [4]IpMask;// Mask

byte [6]MacAddr;// MAC address

byte [4]GwAddr;// Gateway

byte [4]ServAddr;// Server IP

byte RemoteEnable;//Standby

byte [2]Port;// Port

byte Mode;// Mode：0:Server，1:Client

byte DhcpEnable;// DHCP，0:Disable，1:Enable

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update,Type return CCHEX\_RET\_SETNETCFG\_TYPE

Data part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = (anviz\_handle, dev\_idx, ref dev\_info);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgGetByIdx

### Description functions

【Function】Reads the designated short message’s start date, end date, and message content .

### Request

【Mode】int CChex\_MsgGetByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

【Parameter】CchexHandle：,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Idx,Read the short message, Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGGETBYIDX\_UNICODE\_INFO\_TYPE

Data part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int Len; // The length of the following data

byte[5] EmployeeId; // User ID，0 means public short message

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

byte [48\*2]content // Content of short message,UNICODE

### Sample

int ret = CChex\_MsgGetByIdx(anviz\_handle, dev\_idx, msg\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgDelByIdx

### Description functions

【Function】Delete the designated short message

### Request

【Mode】int CChex\_MsgDelByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

【Parameter】CChex\_Start， successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Idx,Delete the designed short message,Input[Parameter]

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGDELBYIDX\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret =CChex\_MsgDelByIdx(anviz\_handle, dev\_idx, msg\_idx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgAddNew

### Description functions

【Function】Add short message.

### Request

【Mode】int CChex\_MsgAddNew(IntPtr CchexHandle, int DevIdx, byte[] Data, int Len);

【Parameter】CChex\_Start，successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data,Short message, Input[Parameter]；

byte[5] EmployeeId; // User ID，0 means public short message

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

byte [48\*2]content // Content of short message,UNICODE

Len,the length of short message，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_MsgAddNew(anviz\_handle, dev\_idx, send\_buff, send\_len);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgGetAllHead

### Description functions

【Function】Read all short message headers.

### Request

【Mode】int CChex\_MsgGetAllHead(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int Len; // All 50 SMS users, start and end time.

byte[5] EmployeeId; // User ID，0 means public SMS

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

...Total 50 records

### Sample

int ret =CChex\_MsgGetAllHead(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_RebootDevice

### Description functions

【Function】Restart the Anviz device

### Request

【Mode】int CChex\_RebootDevice(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_RebootDevice(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_SetTime

### Description functions

【Function】Set date/time of the Anviz device

### Request

【Mode】int CChex\_SetTime(IntPtr CchexHandle, int DevIdx, int Year, int Month, int Day, int Hour, int Min, int Sec);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Year、Month、Day、Hour、 Min、 Sec，Input[Parameter]

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetTime(anviz\_handle, dev\_idx, 2018, 1, 25, 10, 10, 10);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_GetSNConfig

### Description functions

【Function】Get the SN of the Anviz device

### Request

【Mode】int CChex\_GetSNConfig(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]句柄，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[16] sn; // SN，Each number, and it needs to convert into characters

### Sample

int ret = CChex\_GetSNConfig(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadAllRecords

### Description functions

【Function】Download all attendance records.

### Request

【Mode】int CChex\_DownloadAllRecords(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

byte NewRecordFlag; // New or not record?

byte[5] EmployeeId; // User ID，

byte[4] Date; // date/time，The number of seconds apart from 2000.

byte BackId; // Backup ID，the 3 digits; Card，the 2 digits; Password，the 1~0; 11，7~4 digits; 10 Fingerprints（1~10）digits

byte RecordType // Record type，7 digits; 1：open the door ，0：can’t open the door ；3~0 digits attendance status

byte[3] WorkType; // Workcode

byte Rsv // Reserved

### Sample

int ret = CChex\_DownloadAllRecords(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DeleteRecordInfo

### Description functions

【Function】Delete all records, or clear all/ some new records flag.

### Request

【Mode】int CChex\_DeleteRecordInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_RECORD\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；

byte del\_type; // 0:Delete all records；1：Clear all new record flag；2：Clear some records flag，and the deleted number based on del\_count

uint del\_count; // del\_type =2时，assigned clear new records number

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

uint deleted\_count; // How many records or new records flag be deleted?

### Sample

int ret = CChex\_DeleteRecordInfo(anviz\_handle, dev\_idx, ref delete\_record);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetBasicConfigInfo

### Description functions

【Function】Get the basic configuration of the Anviz device

### Request

【Mode】int CChex\_GetBasicConfigInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_BASIC\_CFG\_INFO\_STRU Cfg;

byte[8] software\_version; // firmware version，

uint password; // Password，longest support 6 digits

byte delay\_for\_sleep; // Delay sleep time，0~250 Mins，0 don’t sleep

byte volume; // Volume，0~5，0：mute，5：Max byte language; //Language，0：Simplified Chinese，1：Traditional Chinese，2：English，3.French，4：Spanish，5：Portuguese

byte date\_format; // Date format，0:Chinese，1：UK，2：USA byte time\_format; // Time format，0：24Houes，1：12Hours

byte machine\_status; // Attendance Status，0~15

byte modify\_language; // Modify Language，0x10 You can modify the language of the device.

byte cmd\_version; // Instruction version

### Sample

int ret = CChex\_GetBasicConfigInfo(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.；

## CChex\_SetBasicConfigInfo

### Description functions

【Function】Set the basic configuration of the Anviz device

### Request

【Mode】int CChex\_SetBasicConfigInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_BASIC\_CFG\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；Unmodified fields，0xFF

uint password; // Password，String convert into number

byte pwd\_len; // Password length

byte delay\_for\_sleep; // Delay sleep time，0~250 Mins，0 don’t sleep

byte volume; // Volume，0~5，0：mute，5：Max

byte language; // Language，0：Simplified Chinese，1：Traditional Chinese，2：English，3.French，4：Spanish，5：Portuguese

byte date\_format; // Date format，0:Chinese，1：UK，2：USA

byte time\_format; // Time format，0：24Houes，1：12Hours

byte machine\_status; // Attendance Status，0~15

byte modify\_language; // Modify Language，0x10 You can modify the language of the device.

byte rsv; // Reserved

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetBasicConfigInfo(anviz\_handle, dev\_idx, ref set\_basic\_cfg);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_ListPersonInfo

### Description functions

【Function】Get all user information.

### Request

【Mode】int CChex\_ListPersonInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int CurIdx; // Current index number

int TotalCnt; // The total number of users

byte [5]EmployeeId; // User ID，5 bytes,Longest 12digits

byte password\_len; // Password length

byte max\_password; // Maximum length of password,= 6，unchangeable

int password; // Password

byte max\_card\_id; // The maximum length of the card number，= 6（3bytes）or 10 （4bytes）, unchangeable

uint card\_id; // Card number

byte max\_EmployeeName; // The maximum length of a user's name，= 10、20 、64 and160,unchangeable；=160 ,The user name is stored in EmployeeName2.

byte[64] EmployeeName; // User name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Attendance mode

uint Fp\_Status; // Fingerprint register status，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // Employee Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

### Sample

int ret = CChex\_ListPersonInfo(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_ModifyPersonInfo

### Description functions

【Function】Modify the relevant user’s information.

### Request

【Mode】int CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

person\_num，How many users were changed，Input[Parameter]；

Personlist，user details information，Input[Parameter]；

uint MachineId; // Device ID

int CurIdx; // Current index number

int TotalCnt; // The total number of users

byte [5]EmployeeId; // User ID，5 bytes,Longest 12digits

byte password\_len; // Password length

byte max\_password; // Maximum length of password,= 6，unchangeable

int password; // Password

byte max\_card\_id; // The maximum length of the card number，= 6（3bytes）or 10 （4bytes）, unchangeable

uint card\_id; // Card number

byte max\_EmployeeName; // The maximum length of a user's name，= 10、20 、64 and160,unchangeable；=160 ,The user name is stored in EmployeeName2.

byte[64] EmployeeName; // User name

byte DepartmentId; // Department ID

byte GroupId; // Group

byte Mode; // Attendance mode

uint Fp\_Status; // Fingerprint register status，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User name 2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_ModifyPersonInfo(anviz\_handle, dev\_idx, ref item, 1);

### Notice

1.Make sure that CChex\_Start has been started successfully before run；

## CChex\_DeletePersonInfo

### Description functions

【Function】Deletes the assigned person’s information.

### Request

【Mode】int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_PERSON\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；

byte []EmployeeId; // User ID

byte operation; // Which information be deleted ? The 3 digits: Card; The 2 digits: Password; The 1~0 digits: 1~0 digits ：11; 7~4 digits：10 Fingerprints（1~10）；0xFF: Delete all user’s information .

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_DeletePersonInfo(anviz\_handle, dev\_idx, ref delete\_item);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_DeletePersonInfo\_VER\_4\_NEWID

### Description functions

【Function】Delete the user’s information

(Version:User ID for Chat DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)

### Request

【Mode】int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_EMPLOYEE\_INFO\_STRU\_EXT\_INF\_ID\_VER\_4\_NEWID Config);

【Parameter】CchexHandle：successfully create by CChex\_Start the handle，Input[Parameter]；；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte [28]EmployeeId; // User ID for the String

byte operation; // Delete user Information the 3 bit is card, The 2 bit is Password ,The 0~1 byte is 11 and the 7~14 bit is number of the fingerprints(1~10)； 0xFF，delete all user information

### Response

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_DEL\_EMPLOYEE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [28] EmployeeId; // User ID for the String

### Sample

int ret = CChex\_DeletePersonInfo(anviz\_handle, dev\_idx, ref delete\_item);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadFingerPrint

### Description functions

【Function】Download fingerprint template from Anviz device

### Request

【Mode】int CChex\_DownloadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx,Search the device，Input[Parameter]；

EmployeeId，User ID, Input[Parameter]；

FingerIdx，Fingerprint Indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte []EmployeeId; // User ID

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10

uint fp\_data\_len; // The length of the fingerprint data.

byte []Data; // fingerprint data

### Sample

int ret = CChex\_DownloadFingerPrint(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadFingerPrint\_VER\_4\_NEWID

### Function

【Function】Download the fingerprint information from the device

**(Version:device version DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### Request

【Mode】int CChex\_DownloadFingerPrint\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

EmployeeId: byte[28]User ID，Input[Parameter]; User ID for the String FingerIdx: Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

### Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_DLFINGERPRT\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [28]EmployeeId; // User ID //User ID for the String ID byte[28]

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10

uint fp\_data\_len; // The length of the fingerprint data.

byte []Data; // fingerprint data

### Sample

int ret = CChex\_DownloadFingerPrint\_VER\_4\_NEWID(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_UploadFingerPrint

### Description functions

【Function】Upload fingerprint template to Anviz device

### Request

【Mode】int CChex\_UploadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

EmployeeId，User ID，Input[Parameter]；

FingerId; Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

FingerData，fingerprint data，Input[Parameter]；

DataLen，The length of the fingerprint data，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_DownloadFingerPrint(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_UploadFingerPrint\_VER\_4\_NEWID

### Function

【Function】Upload the fingerprint template to device (Device Type:"FACEPASS7" For :FaceTemplate download )

**(Version:Device Version Model DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### Request

【Mode】int CChex\_UploadFingerPrint\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；；

DevIdx: Index of device，Input[Parameter]；

EmployeeId: User ID，Input[Parameter]; //User ID for the String ID byte[28]

FingerIdx: Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

FingerData，fingerprint data，Input[Parameter]；

DataLen，The length of the fingerprint data，Input[Parameter]；

### Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_ULFINGERPRT\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte []EmployeeId; // /User ID for the String ID byte[28]

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

uint fp\_data\_len; // The length of the fingerprint data

byte []Data; // Fingerprint Data

### Sample

int ret = CChex\_DownloadFingerPrint\_VER\_4\_NEWID(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetTime

### Description functions

【Function】Get the date/time of the Anviz device.

### Request

【Mode】int CChex\_GetTime(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_MSG\_GETTIME\_STRU Cfg;

uint Year; //Year

uint Month; //Month

uint Day; //Day

uint Hour; //Hour

uint Min; //Minute

uint Sec; //Second

### Sample

int ret = CChex\_GetTime(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_InitUserArea

### Description functions

【Function】Initial user area

Initialize all user data areas，Clear all user data, fingerprint data, password/card data.

### Request

【Mode】int CChex\_InitUserArea(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_InitUserArea(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_InitSystem

### Description functions

【Function】initial device

initialize the Anviz device to restore factory Default.

### Request

【Mode】int CChex\_InitSystem(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_InitSystem(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetBasicConfigInfo2

### Description functions

【Function】Get the Anviz device’s configuration2

Get device’s identification precision, fixed wiegand head, wiegand mode, workcode, real-time attendance records , schedule bell , lock control delay, record overflow warning, repeated attendance record time , door sensor delay, schedule bell delay.

### Request

【Mode】int CChex\_GetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF Param;

byte compare\_level; //identification precision

byte wiegand\_range; //fixed wiegand head

byte wiegand\_type; //wiegand mode

byte work\_code; //Workcode function, enable or disable?

byte real\_time\_send; //Realtime function ,enable or disable?

byte auto\_update; //Auto-update function, enable or disable?

byte bell\_lock; //Schedule bell function, enable or disable?

byte lock\_delay; //Lock time delay

uint record\_over\_alarm; //Record overflow alarm

byte re\_attendance\_delay; //Repeat attendance time delay

byte door\_sensor\_alarm; //Door sensor time delay

byte bell\_delay; //Schedule bell time delay

byte correct\_time; //Time calibration

### Sample

int ret = CChex\_GetBasicConfigInfo2(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetBasicConfigInfo2

### Description functions

【Function】Set up the Anviz device’s configuration information2

### Request

【Mode】int CChex\_SetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

config: Input[Parameter]；

byte compare\_level; //identification precision

byte wiegand\_range; //fixed wiegand head

byte wiegand\_type; //wiegand mode

byte work\_code; //Workcode function, enable or disable?

byte real\_time\_send; //Realtime function ,enable or disable?

byte auto\_update; //Auto-update function, enable or disable?

byte bell\_lock; //Schedule bell function, enable or disable?

byte lock\_delay; //Lock time delay

uint record\_over\_alarm; //Record overflow alarm

byte re\_attendance\_delay; //Repeat attendance time delay

byte door\_sensor\_alarm; //Door sensor time delay

byte bell\_delay; //Schedule bell time delay

byte correct\_time; //Time calibration

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetBasicConfigInfo2(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetPeriodTime

### Description functions

【Function】Get time zone from device

Read the timezone information，Total 32 timezones。

### Request

【Mode】int CChex\_GetPeriodTime(IntPtr CchexHandle, int DevIdx, byte SerialNumbe);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

SerialNumbe,timezone number，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day[7]; //One week 7 days,28Byte

byte StartHour; //Start hour

byte StartMin; //Start mins

byte EndHour; //End hour

byte EndMin; //End mins

### Sample

int ret = CChex\_GetPeriodTime(anviz\_handle, dev\_idx,SerialNumbe);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetPeriodTime

### Description functions

【Function】Set timezone

Total 32 timezones。

### Request

【Mode】int CChex\_SetPeriodTime(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_PERIOD\_TIME\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte SerialNumbe;

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day[7]; //one week with 7 days,so should be have 7 groups,28Byte

byte StartHour; //Start Hour

byte StartMin; //Start Mins

byte EndHour; //End Hours

byte EndMin; //End Mins

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetPeriodTime(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run；

## CChex\_GetTeamInfo

### Description functions

【Function】Get Group information

Read one group information, group number 0-16, group0 = normal close; group1=normal open. Only read group2 - group16.

### Request

【Mode】int CChex\_GetTeamInfo(IntPtr CchexHandle, int DevIdx, byte TeamNumbe);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

TeamNumbe:Group number,Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[4] PeriodTimeNumber;//4Group timezone number(refer to 2.29)

### Sample

int ret = CChex\_GetTeamInfo(anviz\_handle, dev\_idx,TeamNumbe);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetTeamInfo

### Description functions

【Function】Setup group

Setup one group, group number 0- 16, group 0= normal close; group1= normal open, only setup group2 -group16.

### Request

【Mode】int CChex\_SetTeamInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_TEAM\_INFO\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte TeamNumbe; //Group Number

byte[4] PeriodTimeNumber; //4Group ,timezone

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetTeamInfo(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_AddFingerprintOnline

### Description functions

【Function】Register fingerprint online

### Request

【Mode】int CCHex\_AddFingerprintOnline(IntPtr CchexHandle, int DevIdx, ref CCHEX\_ADD\_FINGERPRINT\_ONLINE\_STRU\_EXT\_INF Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: Input[Parameter]；

byte[5] EmployeeId; //User ID

byte BackupNum; //Backup number

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_AddFingerprintOnline(anviz\_handle, dev\_idx,ref Param);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.
2. After the recall, the device will register the fingerprint twice, timeout is 10 seconds, the registration error (timeout, operation failure, the user already exists, the fingerprint exists) returned -1, and successfully returns 0.

## CCHex\_ForcedUnlock

### Description functions

【Function】Open the door by software (Force open the lock)

### Request

【Mode】int CCHex\_ForcedUnlock(IntPtr CchexHandle, int DevIdx, ref CCHEX\_FORCED\_UNLOCK\_STRU\_EXT\_INF Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: Input[Parameter]；( Param =IntPtr.Zerohe ; default null pointer , Malaysia panasonic project customization needs to enter Param);

byte LockCmd; //Lock command

byte[5] EmployeeId; //User ID

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_ForcedUnlock(anviz\_handle, DevIdx,IntPtr.Zero);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.；
2. If Not Malaysia Panasonic project customization, Param none pointer..

## CCHex\_Udp\_Search\_Dev

### Description functions

【Function】UDP Research the Anviz device

### Request

【Mode】int CCHex\_Udp\_Search\_Dev(IntPtr CchexHandle);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：(Data length =sizeof(int)+DevNum\*sizeof(CCHEX\_UDP\_SEARCH\_STRU\_EXT\_INF))

int DevNum; // quantity of device, ( =0, No device,data length =4)

CCHEX\_UDP\_SEARCH\_STRU\_EXT\_INF[] dev\_net\_info ; //Device Data(Single 180Byte)

uint MachineId; //Device ID

int Result; //0: ok -1: fail

int DevHardwareType; //device type(0:Normal device;1:support DNS;2:support wifi)

byte[167] Data; //Data(Convert based on device type)

Byte Padding; //Data alignment, padding

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

byte[167] Data: Data type definition

Device type = 0 :Normal device

CCHEX\_UDP\_SEARCH\_STRU BasicSearchInfo; //normal device 63Byte

byte[10] DevType; //device type

byte[16] DevSerialNum; //device serial numebr

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //network mode

byte[8] Version; //Firmware version

byte[4] Reserved; //Reserved

Device type = 1 :Support DNS firmware

CCHEX\_UDP\_SEARCH\_WITH\_DNS\_STRU DnsSearchInfo; //Support DNS firmware 167Byte

CCHEX\_UDP\_SEARCH\_STRU BasicSearchInfo; //device type 0:normal device 63Byte structure

byte[4] Dns; //DNS

byte[100] Url; //URL

Device type = 2 : Support wifi

CCHEX\_UDP\_SEARCH\_TWO\_CARD\_STRU TwocardSearchInfo; \\ support wifi 102Byte

byte[10] DevType; //Device type

byte[16] DevSerialNum; //Device serial number

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //Network mode

byte[8] Version; //Firmware version

byte[4] Reserved; //Reserved

byte CardNumber; //Network card number

CCHEX\_UDP\_SEARCH\_CARD\_STRU CardInfo[2]; //2group network card information: single network card information = 28Byte

byte[10] CardName; //Network card name

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC Address

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

### Sample

int ret = CCHex\_Udp\_Search\_Dev(anviz\_handle);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CCHex\_Udp\_Set\_Dev\_Config

### Description functions

【Function】UDP setting device configuration

### Request

【Mode】int CCHex\_Udp\_Set\_Dev\_Config(IntPtr CchexHandle, ref CCHEX\_UDP\_SET\_DEV\_CONFIG\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

Config: Input[Parameter]；

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC address

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //Network mode

byte[3] Padding; //structure alignment,padding 3byte

uint NewMachineId; //New Device ID

byte[4] Reserved; //Reserved

byte[12] DevUserName; //User name

byte[12] DevPassWord; //Password

int DevHardwareType; //Device type 0:Normal device ;1:support DNS device

byte[4] Dns; //DNS device type = 0 Dns , unchangeable

byte[100] Url; //URL device type = 0 Url,unchangeable

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_Udp\_Set\_Dev\_Config(anviz\_handle,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_ClientConnect

### Description functions

【Function】The client actively connects to the server.

### Request

【Mode】int CCHex\_ClientConnect(IntPtr CchexHandle, byte[] Ip, int Port);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

Ip: Server IP address，Input[Parameter]；

Port: Server Port, Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】Failure:CChex\_Update,Type return CCHEX\_RET\_CLINECT\_CONNECT\_TYPE;

Data Part：

int Result; //-1 err

byte[24] Addr; //IP:Port 如(192.168.100.100:5010)

Successful:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int DevIdx; //

uint MachineId; //Device ID

byte[24] Addr; //IP:Port For example(192.168.100.100:5010)

byte[8] Version; //Version Number

byte[8] DevType; //Device type

int DevTypeFlag; //Type flag

### Sample

int ret = CCHex\_ClientConnect(anviz\_handle,Ip,Port);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_ClientDisconnect

### Description functions

【Function】The client actively disconnects the server.

### Request

【Mode】int CCHex\_ClientDisconnect(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】Failure:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int Result; // -1:error

int DevIdx; //

Successful:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int DevIdx; //Index of device，Input[Parameter]；

uint MachineId; //Device ID

uint Live; //

byte[24] Addr; //ip:Port 如(192.168.100.100:5010)

byte[8] Version; //Version number

byte[8] DevType; //Device type

### Sample

int ret = CCHex\_ClientDisconnect(anviz\_handle,DevIdx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## 2.42 CChex\_GetInfomationCode

### 2.42.1 Description function

【Function】Gets the factory information

Read the factory information ANSI version data:10Byte,UNICODE version data:20Byte

### 2.42.2 Request

【Mode】int CChex\_GetInfomationCode(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.40.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_INFOMATION\_CODE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int fp\_len; //ANSI VERSION:fp\_len == 10 UNICODE VERSION:fp\_len == 20

byte[20] data; //

### 2.42.4 Sample

int ret = CChex\_GetInfomationCode(anviz\_handle, dev\_idx);

### 2.42.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.43 CChex\_SetInfomationCode

### 2.43.1 Description function

【Function】Modify the factory information

Modify the factory information ANSI version data:10Byte ,UNICODE version data:20Byte

### 2.43.2 Request

【Mode】int CChex\_SetInfomationCode(IntPtr CchexHandle, int DevIdx ,byte[] Data, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data: Byte[10] or Byte[20] parameter，Input[Parameter]；

DataLen: Write the parameters based on the version, , ANSI version = 10,UNICODE version = 20, Input[Parameter]；

### 2.43.3Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_INFOMATION\_CODE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.43.4 Sample

int ret = CChex\_SetInfomationCode(anviz\_handle, dev\_idx,Data,DataLen);

### 2.43.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.44 CChex\_GetBellInfo

### 2.44.1 Description function

【Function】Get the Schedule bell information

Read all time of schedule bell，totally 30.

### 2.44.2 Request

【Mode】int CChex\_GetBellInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.44.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_BELL\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_RET\_GET\_BELL\_TIME\_POINT time\_point[30];

byte hour;

byte minute;

byte flag\_week; //Week mark/flag(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

Byte[2] padding; //data structure alignment , invalid data

### 2.44.4 Sample

int ret = CChex\_GetBellInfo(anviz\_handle, dev\_idx);

### 2.44.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.45 CChex\_SetBellInfo

### 2.45.1 Description function

【Function】Setup the schedule bell information

Setup the time of schedule bell

### 2.45.2 Request

【Mode】int CChex\_SetBellInfo(IntPtr CchexHandle, int DevIdx ,byte BellTimeNum,byte Hour,byte Min,byte FlagWeek);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

BellTimeNum：The time to ring the bell，Input[Parameter]；

Hour：Hour，Input[Parameter]；

Min：Minute，Input[Parameter]；

FlagWeek：Week mark/flag(Binary 0000000means：Sat Fri Thu Wed Tue Mon Sun)，Input[Parameter]；

### 2.45.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_BELL\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.45.4 Sample

int ret = CChex\_SetBellInfo(CchexHandle,DevIdx ,BellTimeNum,Hour,Min,FlagWeek);

### 2.45.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.46 CChex\_GetUserAttendanceStatusInfo

### 2.46.1 Description function

【Function】Gets the self-defining attendance status table

Read the information of self-defining attendance status.

### 2.46.2 Request

【Mode】int CChex\_GetUserAttendanceStatusInfo(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.46.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_USER\_ATTENDANCE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int fp\_len; //ANSI VERSION：fp\_len == 80 UNICODE VERSION fp\_len == 160

Byte atten\_status\_number; //Number of attendance status == 8 default

Byte[160] data\_info; //data format: ANSI VERSION: unsigned char [8][10] UNICODE VERSION: unsigned char[8][20] 。

Byte[3] padding; //data structure alignment, invalid data

### 2.46.4 Sample

int ret = CChex\_GetUserAttendanceStatusInfo(anviz\_handle, dev\_idx);

### 2.46.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.47 CChex\_SetUserAttendanceStatusInfo

### 2.47.1 Description function

【Function】Setup the self-defining attendance status

Setup the self-defining attendance status.

### 2.47.2 Request

【Mode】int CChex\_SetUserAttendanceStatusInfo(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_USER\_ATTENDANCE\_STATUS\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：8 groups self-defining status,Input[Parameter]；

uint fp\_len;//ANSI VERSION fp\_len = 80 UNICODE VERSION fp\_len = 160

Byte atten\_status\_number; //Number of attendance status 8 default

Byte[160] data\_info;//ANSI VERSION:8][10]，UNICODE VERSION:[8][20]

Byte[3] padding; //alignment, invalid data

### 2.47.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_USER\_ATTENDANCE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.47.4 Sample

int ret = CChex\_SetUserAttendanceStatusInfo(CchexHandle,DevIdx ,ref Param);

### 2.47.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.48 CChex\_ClearAdministratFlag

### 2.48.1 Description function

【Function】Clear the administrator flag

Clear all administrator flag.

### 2.48.2 Request

【Mode】int CChex\_ClearAdministratFlag(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.48.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_CLEAR\_ADMINISTRAT\_FLAG\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.48.4 Sample

int ret = CChex\_ClearAdministratFlag(anviz\_handle, dev\_idx);

### 2.48.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.49 CChex\_GetSpecialStatus

### 2.49.1 Description function

【Function】Get the special status

Get the current special status. Only for VF30/VP30/T60+

### 2.49.2 Request

【Mode】int CChex\_GetSpecialStatus(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.49.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_SPECIAL\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte status; //Byte1：Door alarm status 0-normal ,status 1-alarm status; Byte5：Door status 0-close , 1-open; Byte6：Door sensor status 0-close, 1-open; Byte7：Lock status 0-close, 1-open

Byte[7] reserved; //reserved useless in the temporary

### 2.49.4 Sample

int ret = CChex\_GetSpecialStatus(anviz\_handle, dev\_idx);

### 2.49.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.50 CChex\_GetAdminCardnumberPassword

### 2.50.1 Description function

【Function】Read administrator card number or password. Only for T5/M5/T50m

Get administrator card number or password.

### 2.50.2 Request

【Mode】int CChex\_GetAdminCardnumberPassword(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.50.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_ADMIN\_CARD\_PWD\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte[13] data; //device type : T5A,T50

\* Parameter :data[13] : if the device type is T5A，so:

DATA Add card ;delete card ;stress/duress card; special information Byte 1-4 5-8 9-12 13

The special information define as below:

Byte 0：Add card

Byte 1：Delete card

Byte 2：Stress/duress

If the device type is T50，so:

DATA Password length+ passwod Reserved

Byte 1-3 4-13

Password length = Byte(1) >> 4

Byte[3] padding; //data structure alignment, invalid data

### 2.50.4 Sample

int ret = CChex\_GetAdminCardnumberPassword(anviz\_handle, dev\_idx);

### 2.50.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.51 CChex\_SetAdminCardnumberPassword

### 2.51.1 Description function

【Function】Setup administrator card or password. Only for T5/M5/T50M

Setup T5A/M5A admin card and T50M admin password.

### 2.51.2 Request

【Mode】int CChex\_SetAdminCardnumberPassword(IntPtr CchexHandle, int DevIdx,byte[] Data, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data[13]：Parameter refer to 2.47 :data[13] description ，Input[Parameter]；

DataLen： length = 13，Input[Parameter]；

### 2.51.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_ADMIN\_CARD\_PWD\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.51.4 Sample

int ret = CChex\_SetAdminCardnumberPassword(CchexHandle,DevIdx,Data,DataLen);

### 2.51.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.52 CChex\_GetDSTParam

### 2.52.1 Description function

【Function】Read the daylight saving time parameters

Read the flag of daylight saving time and time zone .

### 2.52.2Request

【Mode】int CChex\_GetDSTParam(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.52.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_DST\_PARAM\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCCHEX\_SET\_DST\_PARAM\_STRU param; //16byte

byte enabled; //0-Disable 1-enable；

byte ate\_week\_type; //1-Date format 2-week format；

GET\_DST\_PARAM\_TIME start\_time; //7 byte

byte month;

byte day;

byte week\_num; //Weekly definition：0x01-0x04： First 1-4 week 0x81-0x82：Last1-2 week

byte flag\_week; //Week flag: flag\_week 0-6:(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

byte hour;

byte minute;

byte sec;

GET\_DST\_PARAM\_TIME special\_time； //7 byte

### 2.52.4 Sample

int ret = CChex\_GetDSTParam(anviz\_handle, dev\_idx);

### 2.52.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.53 CChex\_SetDSTParam

### 2.53.1 Description function

【Function】Setup daylight saving time

Setup daylight saving time flag and time zone

### 2.53.2 Request

【Mode】int CChex\_SetDSTParam(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DST\_PARAM\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：16byte，Input[Parameter]；

byte enabled; //0-disable 1-enable；

byte ate\_week\_type; //1-Date format 2-week format；

GET\_DST\_PARAM\_TIME start\_time; //7 byte

byte month;

byte day;

byte week\_num; //Weekly definition：0x01-0x04： First 1-4 week 0x81-0x82：Last1-2 week

byte flag\_week; //Week flag: flag\_week 0-6:(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

byte hour;

byte minute;

byte sec;

GET\_DST\_PARAM\_TIME special\_time； //7 byte

### 2.53.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_DST\_PARAM\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.53.4 Sample

int ret = CChex\_SetDSTParam(CchexHandle,DevIdx,ref Param);

### 2.53.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.54 CChex\_GetDevExtInfo

### 2.54.1 Description function

【Function】Gets the device extension information code

Read the factory name/Tax number/factory Address

### 2.54.2 Request

【Mode】int CChex\_GetDevExtInfo(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.54.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_DEV\_EXT\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_SET\_DEV\_EXT\_INFO\_STRU param; //320byte

Byte[50] manufacturer\_name; //Factory name

Byte[100] manufacturer\_addr; //Address

Byte[15] duty\_paragraph; //Tax number

Byte[155] reserved; //Reserved

### 2.54.4 Sample

int ret = CChex\_GetDevExtInfo(CchexHandle,DevIdx);

### 2.54.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.55 CChex\_SetDevExtInfo

### 2.55.1 Description function

【Function】Modify the device extension information code

Modify the factory name/Tax number/factory Address

### 2.55.2 Request

【Mode】int CChex\_SetDevExtInfo(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DEV\_EXT\_INFO\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：320byte，Input[Parameter]；

Byte[50] manufacturer\_name; //factory name

Byte[100] manufacturer\_addr; //factory address

Byte[15] duty\_paragraph; //Tax number

Byte[155] reserved; //Reserved

### 2.55.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_DEV\_EXT\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.55.4 Sample

int ret = CChex\_SetDevExtInfo(CchexHandle,DevIdx,ref Param);

### 2.55.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.56 CChex\_GetBasicConfigInfo3

### 2.56.1Description function

【Function】Get the device configuration information3

Read Wiegand mode。

### 2.56.2 Request

【Mode】int CChex\_GetBasicConfigInfo3(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.56.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_BASIC\_CFG3\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_SET\_BASIC\_CFG\_INFO3\_STRU param; //15 byte

Byte wiegand\_type; //wiegand mode

Byte online\_mode; //online mode

Byte collect\_level; //Acquisition threshold

Byte pwd\_status; //communication password status =0 ,connect don’t need the communication password by TCP/IP; communication password status =1, send 0x04 command, verify the communication password by TCP/IP

Byte sensor\_status; //=0 don’t report the door sensor status; =1 activate report the door sensor status（the device will activate send the response of 0x2F command )

Byte[8] reserved; //Reserved

Byte independent\_time; //User independent time limit

Byte m5\_t5\_status; //= 0 disable; = 1 enable; Out =2, disable In =4 disable，out =5 disable，In

Byte padding; //alignment invalid data

### 2.56.4 Sample

int ret = CChex\_GetBasicConfigInfo3(CchexHandle,DevIdx);

### 2.56.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.57 CChex\_SetBasicConfigInfo3

### 2.57.1 Description function

【Function】Setup the device configuration information3

Read Wiegand mode

### 2.57.2 Request

【Mode】int CChex\_SetBasicConfigInfo3(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_BASIC\_CFG\_INFO3\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config：15byte，Input[Parameter]；

Byte wiegand\_type; //wiegand mode

Byte online\_mode; //Online mode

Byte collect\_level; //Acquisition threshold

Byte pwd\_status; //communication password status =0 ,connect don’t need the communication password by TCP/IP; communication password status =1, send 0x04 command, verify the communication password by TCP/IP

Byte sensor\_status; //=0 don’t report the door sensor status; =1 activate report the door sensor status（the device will activate send the response of 0x2F command )

Byte[8] reserved; //Reserved

Byte independent\_time; //User independent time limit

Byte m5\_t5\_status; //= 0 disable; = 1 enable; Out =2, disable In =4 disable，out =5 disable，In

### 2.57.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_BASIC\_CFG3\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.57.4 Sample

int ret = CChex\_SetBasicConfigInfo3(CchexHandle,DevIdx,ref Config);

### 2.57.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.58 CChex\_ConnectionAuthentication

### 2.58.1 Description function

【Function】connection identification

connection identification, identification successful, then response the other command; if the identification successful and no data transfer in 5 mins , recover to dis-identification mode

### 2.58.2 Request

【Mode】int CChex\_ConnectionAuthentication(IntPtr CchexHandle, int DevIdx,ref CCHEX\_CONNECTION\_AUTHENTICATION\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：24byte，Input[Parameter]；

Byte[12] username;

Byte[12] password;

//Iris user name “admin”，password “admin”，

//Other devices, don’t identify user name, only identify communication password.

### 2.58.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_CONNECTION\_AUTHENTICATION\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.58.4 Sample

int ret = CChex\_ConnectionAuthentication(CchexHandle,DevIdx,ref Param);

### 2.58.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.59 CChex\_GetRecordNumByEmployeeIdAndTime

### 2.59.1 Description function

【Function】Get the record quantity by user ID and time. Only support A20/972 hardware platform devices.

Get the record quantity by user ID and time.

### 2.59.2 Request

【Mode】int CChex\_GetRecordNumByEmployeeIdAndTime(IntPtr CchexHandle, int DevIdx,ref CCHEX\_GET\_RECORD\_INFO\_BY\_TIME Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：13byte，Input[Parameter]；

Byte[5] EmployeeId; //User ID

Byte[4] start\_date; //The number of seconds after 2000.1.2 Byte[4] end\_date; //The number of seconds after 2000.1.2

User ID = 0xFF means all users

Start date = 0xFF, means unlimit the start date

End date = 0xFF, means unlimit the end date

### 2.59.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_NUMBER\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int record\_num; // record quantity

### 2.59.4 Sample

int ret = CChex\_GetRecordNumByEmployeeIdAndTime(CchexHandle,DevIdx,ref Param);

### 2.59.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.60 CChex\_DownloadRecordByEmployeeIdAndTime

### 2.60.1 Description function

【Function】Get the record by user ID and time. Only support A20/972 hardware platform devices.

Get the record by user ID and time。

### 2.60.2 Request

【Mode】int CChex\_DownloadRecordByEmployeeIdAndTime(IntPtr CchexHandle, int DevIdx,ref CCHEX\_GET\_RECORD\_INFO\_BY\_TIME Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：13byte，Input[Parameter]；

Byte[12] EmployeeId; //user ID

Byte[4] start\_date; //The number of seconds after 2000.1.2

Byte[4] end\_date; //The number of seconds after 2000.1.2

User ID = 0xFF means all users

Start date = 0xFF, means unlimit the start date

End date = 0xFF, means unlimit the end date

### 2.60.3Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_BY\_EMPLOYEE\_TIME\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte[5] EmployeeId; //User ID

Byte[4] char date; //date time

Byte char back\_id; //back ID

Byte ecord\_type; //record type

Byte[3] work\_type; //work code

Byte[2] padding; //alignment invalid data

Note: The number of times this type of data is returned based on the number of records recorded during the output download time

### 2.60.4 Sample

int ret = CChex\_DownloadRecordByEmployeeIdAndTime(CchexHandle,DevIdx,ref Param);

### 2.60.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.61 Send attendance records in real time

### 2.61.1 Description function

【Function】Send the records in real time

After verification, the attendance information will be output automatically, and only the response information will be available.

### 2.61.2 Request

【Mode】

【Parameter】

### 2.61.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_LIVE\_SEND\_ATTENDANCE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[5] EmployeeId; //user ID

byte[4] timestamp; //The number of seconds after 2000.1.2

Byte backup; //backup ID

byte record\_type; //record type

byte[3] work\_type[3]; //workcode

byte[2] padding[2];

### 2.61.4Sample

### 2.61.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

2. Set whether the device configuration information 2 is sent in real time

## 2.62 CChex\_GetRecordInfo

### 2.62.1 Description function

【Function】Get the record information

Get the record information, contains already register user quantity, already register FP quantity, already register password quantity, all record quantity and new record quantity

### 2.62.2 Request

【Mode】int CChex\_GetRecordInfoStatus(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.62.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_INFO\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

uint EmployeeNum; //User quantity

uint FingerPrtNum; //FP quantity

uint PasswdNum;

uint CardNum;

uint TotalRecNum;

uint NewRecNum;

### 2.62.4 Sample

int ret = CChex\_GetRecordInfoStatus(CchexHandle,DevIdx);

### 2.62.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.63 CChex\_DownloadAllNewRecords

### 2.63.1 Description function

【Function】Download all record

### 2.63.2Request

【Mode】int CChex\_DownloadAllNewRecords(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.63.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_NEW\_RECORD\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

byte NewRecordFlag; // new record or no

byte[5] EmployeeId; // User ID，

byte[4] Date; // Time，The number of seconds after 2000.1.2

byte BackId; // Backup ID，3 digits：Card，2 digits：，1~0：11，digits 7~4：10 FP templates（1~10）

byte RecordType // Record type，7 digits：1：open the door，0：can’t open the door；3~0 digits attendance status

byte[3] WorkType; // workcode

byte Rsv // reserved

### 2.63.4 Sample

int ret = CChex\_DownloadAllNewRecords(anviz\_handle, dev\_idx);

### 2.63.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.64 Upload user information

【Function】upload user information

### 2.64.2 Request

【Mode】call the universal interface **2.20**  CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

**Call by the device type：dev->DevTypeFlag & 0xff**

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE\_INFO\_STRU EmployeeList, byte EmployeeNum);

ASCII universal：dev->DevTypeFlag & 0xff == 0x02

CChex\_UploadEmployee2Info(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2\_INFO\_STRU

EmployeeList, byte EmployeeNum);

UNICODE universal：dev->DevTypeFlag & 0xff == 0x04

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU

EmployeeList, byte EmployeeNum);

UNICODE\_W2 universal：dev->DevTypeFlag & 0xff == 0x20

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2W2\_INFO\_STRU

EmployeeList, byte EmployeeNum);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

EmployeeNum：Increase the number of employees (8 or 12 per upload per device type and customization)

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CCHEX\_EMPLOYEE\_INFO\_STRU //28byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //password

byte[3] CardId; //card ID

byte[10] EmployeeName; //name

byte DepartmentId; //department ID

byte GroupId; //Group ID

byte Mode; //Attendance mode

byte[2] FpStatus; //FP registration status

byte Special; //Count of the in formations

byte Padding; //Invalid structure alignment

ASCII Universal：dev->DevTypeFlag & 0xff == 0x02

CCHEX\_EMPLOYEE2\_INFO\_STRU //32byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[10] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

Byte[2] Padding; //Invalid structure alignment

UNICODE Universal：dev->DevTypeFlag & 0xff == 0x04

CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU //40byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[20] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //Password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

UNICODE\_W2 Universal：dev->DevTypeFlag & 0xff == 0x20

CCHEX\_EMPLOYEE2W2\_INFO\_STRU

CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU //40byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[20] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //Password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

byte[4] start\_date //Employee starting time，The number of seconds after 2000.1.2

byte[4] end\_date //Employee ending time，The number of seconds after 2000.1.2

### 2.64.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CCHEX\_RET\_ULEMPLOYEE\_INFO\_TYPE

ASCII Universal ：dev->DevTypeFlag & 0xff == 0x02

CCHEX\_RET\_ULEMPLOYEE2\_INFO\_TYPE

UNICODE Universal：dev->DevTypeFlag & 0xff == 0x04

CCHEX\_RET\_ULEMPLOYEE2UNICODE\_INFO\_TYPE

UNICODE\_W2 Universal：dev->DevTypeFlag & 0xff == 0x20

CCHEX\_RET\_ULEMPLOYEE2W2\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.64.4 Sample

int ret = CChex\_UploadEmployeeInfo(anviz\_handle, dev\_idx，EmployeeList，1);

### 2.64.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.65 Chex\_GetBasicConfigInfo5

### 2.65.1 Function

【Function】获取考勤机配置信息5（Bolid定制）

### 2.65.2 Request

【Mode】int CChex\_GetBasicConfigInfo5(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；参；

### 2.65.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_BASIC\_CFG5\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

byte fail\_alarm\_time; // 勤失败报警次数: 0: 不报警1~10 N次失败报警

byte tamper\_alarm; // 防拆报警: 0: 关闭1: 开启

byte[94] reserved; // reserved

### 2.65.4 Sample

int ret = CChex\_GetBasicConfigInfo5(anviz\_handle, dev\_idx);

### 2.65.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.66 CChex\_SetBasicConfigInfo 5

### 2.66.1 Function

【Function】Setup Time attendance device information 5（Bolid Customize）

### 2.66.2 Request

【Mode】int CChex\_SetBasicConfigInfo5(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_BASIC\_CFG\_INFO5\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: //96 byte （0xFF means do not setup）

byte fail\_alarm\_time; // Times of Attendance Fail Alarm: 0: Do not alarm out 1~10 times of alarm out

byte tamper\_alarm; // Tamper alarm: 0: Close1: Active

byte[94] reserved; // reserved

### 2.66.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_BASIC\_CFG5\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

### 2.66.4 Sample

int ret = CChex\_SetBasicConfigInfo5(anviz\_handle, dev\_idx,ref Param);

### 2.66.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

Function

## 2.67 CChex\_GetCardNo

### 2.67.1 Function

【Function】Query T5S swipe card information（Bolid Customize）

**Notice**： 1：The first time call the function ：Setting the device as swipe card mode

2：Swipe card over time > 5sec；

3：The second time call the function ：Return the last Card number before called the function.

### 2.67.2 Request

【Mode】int Chex\_GetCardNo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.67.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_CARD\_ID\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Uint card\_id; //Card Number

### 2.67.4 Sample

int ret = Chex\_GetCardNo(anviz\_handle, dev\_idx);

### 2.67.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.68 CChex\_SetDevCurrentStatus

### 2.68.1 Function

【Function】User to modify the device status by temporary（Bolid Customize）

### 2.68.2 Request

【Mode】int CChex\_SetDevCurrentStatus(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DEV\_CURRENT\_STATUS\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: //96 byte （0xFF means do not setup）

byte alarm\_stop; //Disable the Alarm except 0XFF

byte door\_status //0: Setting the access control as normal 1: Setting the access control as normal Open 2: Setting the access control as normal Close

byte[94] reserved; // reserved

### 2.68.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_DEV\_CURRENT\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

### 2.68.4 Sample

int ret = CChex\_SetDevCurrentStatus(anviz\_handle, dev\_idx,ref Param);

### 2.68.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.69 CChex\_GetServiceURL

### 2.69.1 Function

【Function】Get the server’s URL

### 2.69.2 Request

【Mode】int CChex\_GetServiceURL(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.69.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update return CCHEX\_RET\_GET\_URL\_TYPE

Data Part：

uint MachineId; // device ID

Int Result; // 0:Success -1：Fail

Byte[4] Dns //dns address

byte[100] Url; //URL address

### 2.69.4 Sample

int ret = CChex\_GetServiceURL(anviz\_handle, dev\_idx);

### 2.69.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.70 CChex\_SetServiceURL

### 2.70.1 Function

【Function】Setuphe server’s URL

### 2.70.2 Request

【Mode】int CChex\_SetServiceURL(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_URL\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param: //104 byte

Byte[4] Dns //dns Address

byte[100] Url; //URL Address

### 2.70.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_SET\_URL\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Success -1：Fail

### 2.70.4 Sample

int ret = CChex\_SetServiceURL(anviz\_handle, dev\_idx,ref Param);

### 2.70.15 Notice

1.Make sure the CChex\_Start already active before running

## 2.71 CChex\_UploadFile

### 2.71.1 Function

【Function】Update firmware, Image and Voice

### 2.71.2 Request

【Mode】int CChex\_UploadFile(IntPtr CchexHandle, int DevIdx, byte FileType, byte[] FileName, byte[] Buff, int Len);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

FileType: = 0 Firmware，= 1 Image，= 2 Voice，= 3 Language

FileName: The name update to the device（MAX\_len = 10)；

Buff: The uploaded file is read as a string;

Len： The length of the string of the uploaded file.

### 2.71.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_UPLOADFILE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:Success -1：Fail

uint TotalBytes; // Total length of the uploaded string

uint SendBytes; // Length already uploaded

**Notice：Every 32K of data is uploaded will return the type once SendBytes == TotalBytes，the upload is completed.**

### 2.71.4 Sample

int ret = CChex\_UploadFile(CchexHandle,DevIdx,FileType,FileName,Buff,Len);

### 2.71.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.72 CChex\_UpdateDevStatus

### 2.72.1 Function

【Function】ask device the status of the firmware updating

**Notice:** After the upgrade package is uploaded, it is called multiple times. When the result is: 1: Check completion 2: The verification is successful. You can restart the upgrade

### 2.72.2 Request

【Mode】int CChex\_UpdateDevStatus(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.72.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_UPDATEFILE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Success -1：Fail

int verify\_status; // 0:verifying ;1: Verify Success

int verify\_ret; // 0:Verify Success;1: Verify Fail

### 2.72.4 Sample

int ret = CChex\_UpdateDevStatus(anviz\_handle, dev\_idx);

### 2.72.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.73 CChex\_GetStatusSwitch

### 2.73.1 Function

【Function】Get status switch information, total with 16 status

**Notice：Device TypeDevTypeFlag & 0x200000 = = 1 can be called**

### 2.73.2 Request

【Mode】int CChex\_GetStatusSwitch(IntPtr CchexHandle, int DevIdx,byte GroupId);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

GroupId：Edit Group ID

### 2.73.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_STATUS\_SWITCH\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

byte group\_id; //get the group number

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day\_week[7]; //7 groups as 7day for one week. One group with 28Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[2] padding; //Invalid data, fill in the structure

### 2.73.4 Sample

int ret = CChex\_GetStatusSwitch(anviz\_handle, dev\_idx,GroupId);

### 2.73.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.74 CChex\_SetStatusSwitch

### 2.74.1 Function

【Function】Setup status switch information, total with 16 status

**Notice：Device Type DevTypeFlag & 0x200000 = = 1 can be called**

### 2.74.2 Request

【Mode】int CChex\_SetStatusSwitch(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_STATUS\_SWITCH\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param： // 32 byte

byte group\_id; //get the group number

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day\_week[7]; // 7 groups as 7day for one week. One group with 28Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[2] padding; //Invalid data, fill in the structure

### 2.74.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_STATUS\_SWITCH\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

### 2.74.4 Sample

int ret = CChex\_SetStatusSwitch(anviz\_handle, dev\_idx,ref Param);

### 2.74.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.75 CChex\_GetStatusSwitch\_EXT

### 2.75.1 Function

【Function】Get status switch information

**Notice：Device TypeDev TypeFlag & 0x100000 = = 1 can be called**

### 2.75.2 Request

【Mode】int CChex\_GetStatusSwitch\_ext(IntPtr CchexHandle, int DevIdx,byte FlagWeek);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

FlagWeek：Week day as 0-6，to represent Sun. to Sat., Such as Monday ：00000010

### 2.75.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_GET\_STATUS\_SWITCH\_EXT\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

byte flag\_week; //get the group number

CCHEX\_ONE\_TIMER\_STATUS one\_time[8]; //8 time zone 40Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[3] padding; //Invalid data, fill in the structure

### 2.75.4 Sample

int ret = CChex\_GetStatusSwitch\_EXT(anviz\_handle, dev\_idx,flag\_week);

### 2.75.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.76 CChex\_SetStatusSwitch\_EXT

### 2.76.1 Function

【Function】Setup time attendance status information

**Notic：Device type DevTypeFlag & 0x100000 = = 1 can be call**

### 2.76.2 Request

【Mode】int CChex\_SetStatusSwitch\_EXT(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_STATUS\_SWITCH\_STRU\_EXT Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param： // 44 byte

byte flag\_week; //get the group number

CCHEX\_ONE\_TIMER\_STATUS one\_time[8]; //8 timezone 40Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[3] padding; //Invalid data, fill in the structure

### 2.76.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_SET\_STATUS\_SWITCH\_EXT\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

### 2.76.4 Sample

int ret = CChex\_SetStatusSwitch\_EXT(anviz\_handle, dev\_idx,ref Param);

### 2.76.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.77 CChex\_Get\_Service\_Port

### 2.77.1 Function

【Function】Setup the current server port

### 2.77.2 Request

【Mode】int CChex\_Get\_Service\_Port(IntPtr CchexHandle);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

### 2.77.3 Sample

int ret = CChex\_Get\_Service\_Port(CchexHandle);

【Return value】Returnret as server port

## 2.78 CChex\_SetSdkConfig

### 2.78.1 Function

【Function】Monitor the records status, the new record will automatic download and after download new records automatic to make a flag and SDK will print out to the LOG folder.

\* after CChex\_Start();

\* para :

\* SetRecordflag = 1 set recordflag after download new record;else = 0

\* SetLogFile = 1 set some info log to file for find problem ;else = 0

\* if do not set "CChex\_SetSdkConfig(void \*CchexHandle,int SetAutoDownload,int SetRecordflag,int SetLogFile)", config is default

\* ANVIZ\_DEFAULT:

\* W2 : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

\* SEATS : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

\* DR : SetRecordflag = 0,SetLogFile = 0,SetAutodownload = 1;

\* COMMON : SetRecordflag = 0,SetLogFile = 0,SetAutodownload = 1;

\* Bolid : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

### 2.78.2 Request

【Mode】void CChex\_SetSdkConfig(IntPtr CchexHandle, int SetAutoDownload,int SetRecordflag, int SetLogFile);

【Parameter】SetAutodownload: = 1: Monitor records status , when get new records automatic download record,others do not download automatic

SetRecordflag: = 1:After download new records automatic to make a flag.

SetLogFile: = 1:SDK Print out to Log file

### 2.78.3 Sample

int ret = CChex\_SetSdkConfig(CchexHandle,1,1,0);

;

## 2.79 CChex\_UploadRecord

### 2.79.1 Function

【Function】Upload Time Attendance Records

### 2.79.2 Request

【Mode】int CChex\_UploadRecord(IntPtr CchexHandle, int DevIdx, ref CCHEX\_UPLOAD\_RECORD\_INFO\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[5] EmployeeId; //Employee Id

Byte[4] char date; //Date

Byte char back\_id; //Backup ID

Byte ecord\_type; //Record Type

Byte[3] work\_type; //Work Code

### 2.79.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_UPLOAD\_RECORD\_TYPE //87

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Byte[5] EmployeeId; // digital of Employee Id

Byte[3] padding; // 无效数据结构对齐

### 2.79.4 Sample

int ret = CChex\_UploadRecord(anviz\_handle, dev\_idx,ref Param);

### 2.79.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.80 CChex\_UploadRecord\_VER\_4\_NEWID

### 2.80.1 Function

【Function】Upload Time Attendance Records

**(Version: Device Type DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### 2.80.2 Request

【Mode】int CChex\_UploadRecord\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, ref CCHEX\_UPLOAD\_RECORD\_INFO\_STRU\_VER\_4\_NEWID Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[28] EmployeeId; // String of Employee Id

Byte[4] date; //Date

Byte back\_id; //Backup ID

Byte ecord\_type; //Record Type

Byte[3] work\_type; //Work Code

### 2.80.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_UPLOAD\_RECORD\_TYPE //87

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Byte[28] EmployeeId; // String of Employee Id

### 2.80.4 Sample

int ret = CChex\_UploadRecord\_VER\_4\_NEWID(anviz\_handle, dev\_idx,ref Param);

### 2.80.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.81 CChex\_GetOnePersonInfo

**(Version :digital of Employee Id )**

## CChex\_GetOnePersonInfo\_VER\_4\_NEWID

**(Version:**

**String of Employee Id DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### 2.81.1 Function

【Function】According to employee Id to get user information

### 2.81.2 Request

【Mode】int CChex\_GetOnePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_ONE\_EMPLOYEE\_INFO\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[5] EmployeeId; //digital of Employee Id

【Mode】int CChex\_GetOnePersonInfo\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_ONE\_EMPLOYEE\_INFO\_STRU\_VER\_4\_NEWID Param);

**(Version :Device Version DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[28] EmployeeId; //String of Employee Id

### 2.81.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_ONE\_EMPLOYEE\_INFO\_TYPE //88

Data Part：

**digital of Employee Id ,Without employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [5]EmployeeId; // User ID 5 bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

**digital of Employee Id ,With employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [5]EmployeeId; // User ID 5 bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

byte[4] start\_date; // RFC Information

byte[4] end\_date; // CURP Information

**String of Employee Id , with employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [28]EmployeeId; // Enployee ID,28bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

byte[4] start\_date; // RFC Information

byte[4] end\_date; // CURP Information

### 2.81.4 Sample

int ret = CChex\_UploadRecord(anviz\_handle, dev\_idx,ref Param);

int ret = CChex\_UploadRecord\_VER\_4\_NEWID(anviz\_handle, dev\_idx,ref Param);

### 2.81.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.82 CChex\_GetMachineId

### 2.82.1 Function

【Function】Read the device communication device ID

### 2.82.2 Request

【Mode】int CChex\_GetMachineId(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.82.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_MACHINE\_ID\_TYPE //84

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

uint cur\_machineid; //Communicatrion device ID

### 2.82.4 Sample

int ret = CChex\_GetMachineId(anviz\_handle, dev\_idx);

### 2.82.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.83 CChex\_SetMachineId

### 2.83.1 Function

【Function】Setting device Communication device ID

### 2.83.2 Request

【Mode】int CChex\_SetMachineId(IntPtr CchexHandle, int DevIdx,uint MachineId);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

MachineId: device Communication device ID;

### 2.83.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_MACHINE\_ID\_TYPE //85

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

uint cur\_machineid; //New Communicatrion device ID

uint old\_machineid; //Old Communicatrion device ID

### 2.83.4 Sample

int ret = CChex\_SetMachineId(anviz\_handle, dev\_idx,MachineId);

### 2.83.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.84 CChex\_ManageLogRecord

### 2.84.1 Function

【Function】Setting device Communication device ID

### 2.84.2 Request

【Mode】int CChex\_ManageLogRecord(IntPtr CchexHandle, int DevIdx, ref CCHEX\_MANAGE\_LOG\_RECORD Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[4] start\_date; // The second since of after 2000 years, 2000.1.2

Byte[4] end\_date; //The second since of after 2000 years, 2000.1.2

Byte CmdType; //Extended command ：　0x00 Get the total number of current time periods

0x01 Download the current time period log record

0x02 delete all records in the current time period

0x03 Set real-time report log record

0x04 Get the status of real-time reporting records

Byte AutoFlag; //0:Close real-time report log record 1: Enable real-time report log record

### 2.84.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_MANAGE\_LOG\_RECORD\_TYPE //90

Data Part：

uint MachineId; // Device ID

uint CmdType; // Extended command

0x00 :Result judge success,TotalNum is Total number of the log

0x02 :Result is valid Delete success or not

0x03 Set real-time report log record

0x04 Get the status of real-time reporting records

0x05 Real-time reporting record

Int Result; // 0:Succes -1：Failure

uint IsAuto; // Auto-tagging

uint TotalNum; // Total number of the log

CmdType == 0x00:Result==0 Total number of the log

CmdType == 0x01:Result==0 Total download number of the log

uint CurNum; // The log id of the current logByte[5] EmployeeId; //Employee Id

Byte[4] Date; //Event date The second since of after 2000 years, 2000.1.2

Byte[2] LogType; //Log Type 0x0001 open door 0x0002 close door

0x0003 door sensor 0x0004 Tamper alarm

0x0005 Exit button 0x0006 burst open the door

Byte[2] LogLen; //Log content length

Byte[3] padding; //Fill alignment invalid data

### 2.84.4 Sample

int ret = CChex\_ManageLogRecord(anviz\_handle, dev\_idx,ref Param);

### 2.84.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

# Return value

1：Success；

-1：Parameter Error；

-2：Lack of device resources；

-3：Unknown Error；

# Overview

## Introduction

This API document mainly defines the development interface of the Anviz SDK, which provides reference for developers to connect and operate related devices.

This document is mainly related to the software development engineers, software testing engineers and project managers.

## Overview of functions

This API document mainly provides some interfaces of the client/server to the PC end, getting the parameters of the time attendance/access control, and setting the configuration and parameters of the time attendance/access control device. In order to support multiple devices, the interfaces between queries and settings exist asynchronously. SDK is compiled into the form of a dynamic library.

## System logic structure

Device

PC

CChex\_Init

CChex\_Start

CChex\_Stop

Start

CChex\_GetNetConfig

CChex\_SetNetConfig

CChex\_Update

SDK

SetNetwork

GetNetwork

Result

Stop

## Brief introduction of interface functions

uint CChex\_Version();

void CChex\_Init();

IntPtr CChex\_Start();

void CChex\_Stop(IntPtr CchexHandle);

int CChex\_Update(IntPtr CchexHandle, int[] DevIdx, int[] Type, IntPtr Buff, int Len);

int CChex\_GetNetConfig(IntPtr CchexHandle, int DevIdx);

int CChex\_SetNetConfig(IntPtr CchexHandle, int DevIdx, ref CCHEX\_NETCFG\_INFO\_STRU Config);

int CChex\_MsgGetByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

int CChex\_MsgDelByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

int CChex\_MsgAddNew(IntPtr CchexHandle, int DevIdx, byte[] Data, int Len);

int CChex\_MsgGetAllHead(IntPtr CchexHandle, int DevIdx);

int CChex\_RebootDevice(IntPtr CchexHandle, int DevIdx);

int CChex\_SetTime(IntPtr CchexHandle, int DevIdx, int Year, int Month, int Day, int Hour, int Min, int Sec);

int CChex\_GetSNConfig(IntPtr CchexHandle, int DevIdx);

int CChex\_DownloadAllRecords(IntPtr CchexHandle, int DevIdx);

int CChex\_DeleteRecordInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_RECORD\_INFO\_STRU Config);

int CChex\_GetBasicConfigInfo(IntPtr CchexHandle, int DevIdx);

int CChex\_SetBasicConfigInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_BASIC\_CFG\_INFO\_STRU Config);

int CChex\_ListPersonInfo(IntPtr CchexHandle, int DevIdx);

int CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_PERSON\_INFO\_STRU Config);

int CChex\_DownloadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

int CChex\_UploadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

int CChex\_GetTime(IntPtr CchexHandle, int DevIdx);//(24)

int CChex\_InitUserArea(IntPtr CchexHandle, int DevIdx);

int CChex\_InitSystem(IntPtr CchexHandle, int DevIdx);

int CChex\_GetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx);

int CChex\_SetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF config);

int CChex\_GetPeriodTime(IntPtr CchexHandle, int DevIdx, byte SerialNumbe);

int CChex\_SetPeriodTime(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_PERIOD\_TIME\_STRU\_EXT\_INF config);

int CChex\_GetTeamInfo(IntPtr CchexHandle, int DevIdx, byte TeamNumbe);

int CChex\_SetTeamInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_TEAM\_INFO\_STRU\_EXT\_INF config);

int CCHex\_AddFingerprintOnline(IntPtr CchexHandle, int DevIdx, ref CCHEX\_ADD\_FINGERPRINT\_ONLINE\_STRU\_EXT\_INF Param);

int CCHex\_ForcedUnlock(IntPtr CchexHandle, int DevIdx, ref CCHEX\_FORCED\_UNLOCK\_STRU\_EXT\_INF Param);

int CCHex\_Udp\_Search\_Dev(IntPtr CchexHandle);

int CCHex\_Udp\_Set\_Dev\_Config(IntPtr CchexHandle, ref CCHEX\_UDP\_SET\_DEV\_CONFIG\_STRU\_EXT\_INF config);

int CCHex\_ClientConnect(IntPtr CchexHandle, byte[] Ip, int Port);

int CCHex\_ClientDisconnect(IntPtr CchexHandle, int DevIdx);

## Message Type

CChex\_Update(anviz\_handle, dev\_idx, Type, pBuff, len);

You need to loop the query to see if there is an asynchronous return, and if you have a different Type of data parsing, get the data you want.public enum MsgType:int

{

CCHEX\_RET\_RECORD\_INFO\_TYPE = 1

, CCHEX\_RET\_DEV\_LOGIN\_TYPE

, CCHEX\_RET\_DEV\_LOGOUT\_TYPE

, CCHEX\_RET\_DLFINGERPRT\_TYPE = 4

, CCHEX\_RET\_ULFINGERPRT\_TYPE

, CCHEX\_RET\_MODIFY\_PERSON\_INFO\_TYPE = 8

, CCHEX\_RET\_LIST\_PERSON\_INFO\_TYPE

, CCHEX\_RET\_MSGGETBYIDX\_INFO\_TYPE = 12

, CCHEX\_RET\_MSGGETBYIDX\_UNICODE\_INFO\_TYPE

, CCHEX\_RET\_MSGADDNEW\_INFO\_TYPE

, CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

, CCHEX\_RET\_MSGDELBYIDX\_INFO\_TYPE // 15

, CCHEX\_RET\_MSGGETALLHEAD\_INFO\_TYPE

, CCHEX\_RET\_REBOOT\_TYPE

, CCHEX\_RET\_DEV\_STATUS\_TYPE

, CCHEX\_RET\_MSGGETALLHEADUNICODE\_INFO\_TYPE

, CCHEX\_RET\_SETTIME\_TYPE // 20

, CCHEX\_RET\_UPLOADFILE\_TYPE

, CCHEX\_RET\_GETNETCFG\_TYPE

, CCHEX\_RET\_SETNETCFG\_TYPE

, CCHEX\_RET\_GET\_SN\_TYPE //24

, CCHEX\_RET\_GET\_BASIC\_CFG\_TYPE = 29

, CCHEX\_RET\_SET\_BASIC\_CFG\_TYPE

, CCHEX\_RET\_DEL\_PERSON\_INFO\_TYPE = 31

, CCHEX\_RET\_DEL\_RECORD\_OR\_FLAG\_INFO\_TYPE = 33

,CCHEX\_RET\_GET\_BASIC\_CFG2\_TYPE = 37

,CCHEX\_RET\_SET\_BASIC\_CFG2\_TYPE = 38

,CCHEX\_RET\_GETTIME\_TYPE = 39

,CCHEX\_RET\_INIT\_USER\_AREA\_TYPE = 40

,CCHEX\_RET\_INIT\_SYSTEM\_TYPE = 41

,CCHEX\_RET\_GET\_PERIOD\_TIME\_TYPE = 42

,CCHEX\_RET\_SET\_PERIOD\_TIME\_TYPE = 43

,CCHEX\_RET\_GET\_TEAM\_INFO\_TYPE = 44

,CCHEX\_RET\_SET\_TEAM\_INFO\_TYPE = 45

,CCHEX\_RET\_ADD\_FINGERPRINT\_ONLINE\_TYPE = 46

,CCHEX\_RET\_FORCED\_UNLOCK\_TYPE = 47

,CCHEX\_RET\_UDP\_SEARCH\_DEV\_TYPE = 48

,CCHEX\_RET\_UDP\_SET\_DEV\_CONFIG\_TYPE = 49

,CCHEX\_RET\_GET\_INFOMATION\_CODE\_TYPE = 50

,CCHEX\_RET\_SET\_INFOMATION\_CODE\_TYPE = 51

,CCHEX\_RET\_GET\_BELL\_INFO\_TYPE = 52

,CCHEX\_RET\_SET\_BELL\_INFO\_TYPE = 53

,CCHEX\_RET\_LIVE\_SEND\_ATTENDANCE\_TYPE = 54

,CCHEX\_RET\_GET\_USER\_ATTENDANCE\_STATUS\_TYPE = 55

,CCHEX\_RET\_SET\_USER\_ATTENDANCE\_STATUS\_TYPE = 56

,CCHEX\_RET\_CLEAR\_ADMINISTRAT\_FLAG\_TYPE = 57

,CCHEX\_RET\_GET\_SPECIAL\_STATUS\_TYPE = 58

,CCHEX\_RET\_GET\_ADMIN\_CARD\_PWD\_TYPE = 59

,CCHEX\_RET\_SET\_ADMIN\_CARD\_PWD\_TYPE = 60

,CCHEX\_RET\_GET\_DST\_PARAM\_TYPE = 61

,CCHEX\_RET\_SET\_DST\_PARAM\_TYPE = 62

,CCHEX\_RET\_GET\_DEV\_EXT\_INFO\_TYPE = 63

,CCHEX\_RET\_SET\_DEV\_EXT\_INFO\_TYPE = 64

,CCHEX\_RET\_GET\_BASIC\_CFG3\_TYPE = 65

,CCHEX\_RET\_SET\_BASIC\_CFG3\_TYPE = 66

,CCHEX\_RET\_CONNECTION\_AUTHENTICATION\_TYPE = 67

,CCHEX\_RET\_GET\_RECORD\_NUMBER\_TYPE = 68

,CCHEX\_RET\_GET\_RECORD\_BY\_EMPLOYEE\_TIME\_TYPE = 69

,CCHEX\_RET\_GET\_RECORD\_INFO\_STATUS\_TYPE = 70

,CCHEX\_RET\_GET\_NEW\_RECORD\_INFO\_TYPE = 71

,CCHEX\_RET\_ULEMPLOYEE2W2\_INFO\_TYPE = 72,

CCHEX\_RET\_GET\_BASIC\_CFG5\_TYPE = 73,

CCHEX\_RET\_SET\_BASIC\_CFG5\_TYPE = 74,

CCHEX\_RET\_GET\_CARD\_ID\_TYPE = 75,

CCHEX\_RET\_SET\_DEV\_CURRENT\_STATUS\_TYPE = 76,

CCHEX\_RET\_GET\_URL\_TYPE = 77,

CCHEX\_RET\_SET\_URL\_TYPE = 78,

CCHEX\_RET\_GET\_STATUS\_SWITCH\_TYPE = 79,

CCHEX\_RET\_SET\_STATUS\_SWITCH\_TYPE = 80,

CCHEX\_RET\_GET\_STATUS\_SWITCH\_EXT\_TYPE = 81,

CCHEX\_RET\_SET\_STATUS\_SWITCH\_EXT\_TYPE = 82,

CCHEX\_RET\_UPDATEFILE\_STATUS\_TYPE = 83,

,CCHEX\_RET\_CLINECT\_CONNECT\_TYPE = 200

,CCHEX\_RET\_CLINECT\_DISCONNECT\_TYPE = 201

};

## Setup label and print setup Description

Generic version:

Default Setup: After download new records mark as:0(NO) Print LOG:0(NO)

W2 Version：

Default Setup: After download new records mark as:1(Yes) Print LOG:0(NO)

Customize(S) Version：

Default Setup: After download new records mark as:1(Yes) Print LOG:0(NO)

Customize（F）Version：：

Default Setup: After download new records mark as:0(NO) Print LOG:0(NO)

Change Configuration path:

1：Defining the configuration file：tc-b\_new\_sdk.ini

[LogFile]

LogFile = 1 1：yes 0：no

[SetRecordFlag]

SetRecordFlag = 1 1：yes 0：no

[Debug]

Debug = 0

2:Call the function interface：void CChex\_SetSdkConfig(void \*CchexHandle,int SetRecordflag,int SetLogFile);

Parameter：

int SetRecordflag 1：yes 0：no

int SetLogFile 1：yes 0：no

Priority level:

High： Call the function interface

High： Defining the configuration file

Low： Defining Setup

Notice：When without any “Call the function interface” and “Defining the configuration file as “Defining Setup”

# Description interface

## CChex\_Version

### Description functions

【Function】Query SDK Version.

### Request

【Mode】uint CChex\_Version()

【Parameter】None

### Response

【Return value】Get SDK version, Returns the version number of an integer number.

### Sample

int sdk\_ver = CChex\_Version();

### Notice

## CChex\_Init

### Description functions

【Function】 The SDK function initializes and initializes the socket application interface.

### Request

【Mode】void CChex\_Init()

【Parameter】None

### Response

【Return value】None

### Sample

CChex\_Init();

### Notice

None

## CChex\_Start

### Description functions

【Function】 Start the SDK, allocate space, and establish communication with the Anviz device.

### Request

【Mode】IntPtr CChex\_Start()

【Parameter】None

### Response

【Return value】Return the handle of SDK.

### Sample

IntPtr sdk\_handle = CChex\_Start();

if (sdk\_handle != null)

{

MessageBox.Show("Startup OK");

｝ else

{

MessageBox.Show("Startup errors,Please restart the program.");

}

### Notice

1. Make sure that CChex\_Init is initialized before run.

## CChex\_Stop

### Description functions

【Function】Stop the SDK, release the space, close the socket chain and so on.

### Request

【Mode】void CChex\_Stop(IntPtr CchexHandle)

【Parameter】CchexHandle,CChex\_Start successfully create the handle

### Response

【Return value】None

### Sample

CChex\_stop();

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_Update

### Description functions

【Function】The Return value get or set asynchronously.。

### Request

【Mode】int CChex\_Update(IntPtr CchexHandle, int[] DevIdx, int[] Type, IntPtr Buff, int Len);

【Parameter】CchexHandle,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx,Device index returned asynchronously,Output[Parameter]；

Buff,Returned data section,Output [Parameter]；

Len,Returns the length of the data section,Input[Parameter]；

### Response

【Return value】> 0：Successful asynchronous ; Return value == 0：Invalid Return value；< 0：buffer space is not enough，based on Return value, then re-apply the space.

### Sample

int ret = CChex\_Update(anviz\_handle, dev\_idx, Type, pBuff, len);

if (ret > 0)

{

switch(Type)

{

case CCHEX\_RET\_DEV\_LOGIN\_TYPE: // Connect the Anviz device successfully and return the Device ID, Device IP address, Software version, Device type and software version, etc.

break;

case CCHEX\_RET\_GET\_BASIC\_CFG\_TYPE: // Some basic information about the Anviz device, such as administrator password, firmware version, volume, etc.

break;

case CCHEX\_RET\_DEV\_STATUS\_TYPE: // Total number of employees, total number of fingerprints, total number of passwords, total number of cards, total attendance records, total new attendance record.

default:

break;

}

}else if (ret == 0)

{

// invalid data

}else

{

// Buff is not enough,

}

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetNetConfig

### Description functions

【Function】Query Anviz device’s network Configuration

### Request

【Mode】int CChex\_GetNetConfig(IntPtr CchexHandle, int DevIdx);

【Parameter】CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx,search the device Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GETNETCFG\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [4]IpAddr;// IP address

byte [4]IpMask;// Mask

byte [6]MacAddr;// MAC

byte [4]GwAddr;// Gateway

byte [4]ServAddr;// Sever IP address

byte RemoteEnable;//Standby

byte [2]Port;// Port

byte Mode;// Mode：0: Server，1:Client

byte DhcpEnable;// DHCP，0:Disable，1:Enable

### Sample

int ret = CChex\_GetNetConfig();

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetNetConfig

### Description functions

【Function】Set the network configuration of the Anviz device.

### Request

【Mode】int CChex\_SetNetConfig(IntPtr CchexHandle, int DevIdx, ref CCHEX\_NETCFG\_INFO\_STRU Config);

【Parameter】CchexHandle：,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config:

byte [4]IpAddr;// IP Address

byte [4]IpMask;// Mask

byte [6]MacAddr;// MAC address

byte [4]GwAddr;// Gateway

byte [4]ServAddr;// Server IP

byte RemoteEnable;//Standby

byte [2]Port;// Port

byte Mode;// Mode：0:Server，1:Client

byte DhcpEnable;// DHCP，0:Disable，1:Enable

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update,Type return CCHEX\_RET\_SETNETCFG\_TYPE

Data part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = (anviz\_handle, dev\_idx, ref dev\_info);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgGetByIdx

### Description functions

【Function】Reads the designated short message’s start date, end date, and message content .

### Request

【Mode】int CChex\_MsgGetByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

【Parameter】CchexHandle：,CChex\_Start successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Idx,Read the short message, Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGGETBYIDX\_UNICODE\_INFO\_TYPE

Data part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int Len; // The length of the following data

byte[5] EmployeeId; // User ID，0 means public short message

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

byte [48\*2]content // Content of short message,UNICODE

### Sample

int ret = CChex\_MsgGetByIdx(anviz\_handle, dev\_idx, msg\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgDelByIdx

### Description functions

【Function】Delete the designated short message

### Request

【Mode】int CChex\_MsgDelByIdx(IntPtr CchexHandle, int DevIdx, byte Idx);

【Parameter】CChex\_Start， successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Idx,Delete the designed short message,Input[Parameter]

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGDELBYIDX\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret =CChex\_MsgDelByIdx(anviz\_handle, dev\_idx, msg\_idx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgAddNew

### Description functions

【Function】Add short message.

### Request

【Mode】int CChex\_MsgAddNew(IntPtr CchexHandle, int DevIdx, byte[] Data, int Len);

【Parameter】CChex\_Start，successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data,Short message, Input[Parameter]；

byte[5] EmployeeId; // User ID，0 means public short message

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

byte [48\*2]content // Content of short message,UNICODE

Len,the length of short message，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_MsgAddNew(anviz\_handle, dev\_idx, send\_buff, send\_len);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_MsgGetAllHead

### Description functions

【Function】Read all short message headers.

### Request

【Mode】int CChex\_MsgGetAllHead(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int Len; // All 50 SMS users, start and end time.

byte[5] EmployeeId; // User ID，0 means public SMS

byte StartYear; // Start time Year

byte StartMonth; // Start time Month

byte StartDay; // Start time Day

byte EndYear; // End time Year

byte EndMonth; // End time Month

byte EndDay; // End time Day

...Total 50 records

### Sample

int ret =CChex\_MsgGetAllHead(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_RebootDevice

### Description functions

【Function】Restart the Anviz device

### Request

【Mode】int CChex\_RebootDevice(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_RebootDevice(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_SetTime

### Description functions

【Function】Set date/time of the Anviz device

### Request

【Mode】int CChex\_SetTime(IntPtr CchexHandle, int DevIdx, int Year, int Month, int Day, int Hour, int Min, int Sec);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Year、Month、Day、Hour、 Min、 Sec，Input[Parameter]

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetTime(anviz\_handle, dev\_idx, 2018, 1, 25, 10, 10, 10);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.已经成功启动；

## CChex\_GetSNConfig

### Description functions

【Function】Get the SN of the Anviz device

### Request

【Mode】int CChex\_GetSNConfig(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]句柄，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[16] sn; // SN，Each number, and it needs to convert into characters

### Sample

int ret = CChex\_GetSNConfig(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadAllRecords

### Description functions

【Function】Download all attendance records.

### Request

【Mode】int CChex\_DownloadAllRecords(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

byte NewRecordFlag; // New or not record?

byte[5] EmployeeId; // User ID，

byte[4] Date; // date/time，The number of seconds apart from 2000.

byte BackId; // Backup ID，the 3 digits; Card，the 2 digits; Password，the 1~0; 11，7~4 digits; 10 Fingerprints（1~10）digits

byte RecordType // Record type，7 digits; 1：open the door ，0：can’t open the door ；3~0 digits attendance status

byte[3] WorkType; // Workcode

byte Rsv // Reserved

### Sample

int ret = CChex\_DownloadAllRecords(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DeleteRecordInfo

### Description functions

【Function】Delete all records, or clear all/ some new records flag.

### Request

【Mode】int CChex\_DeleteRecordInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_RECORD\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；

byte del\_type; // 0:Delete all records；1：Clear all new record flag；2：Clear some records flag，and the deleted number based on del\_count

uint del\_count; // del\_type =2时，assigned clear new records number

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

uint deleted\_count; // How many records or new records flag be deleted?

### Sample

int ret = CChex\_DeleteRecordInfo(anviz\_handle, dev\_idx, ref delete\_record);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetBasicConfigInfo

### Description functions

【Function】Get the basic configuration of the Anviz device

### Request

【Mode】int CChex\_GetBasicConfigInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_BASIC\_CFG\_INFO\_STRU Cfg;

byte[8] software\_version; // firmware version，

uint password; // Password，longest support 6 digits

byte delay\_for\_sleep; // Delay sleep time，0~250 Mins，0 don’t sleep

byte volume; // Volume，0~5，0：mute，5：Max byte language; //Language，0：Simplified Chinese，1：Traditional Chinese，2：English，3.French，4：Spanish，5：Portuguese

byte date\_format; // Date format，0:Chinese，1：UK，2：USA byte time\_format; // Time format，0：24Houes，1：12Hours

byte machine\_status; // Attendance Status，0~15

byte modify\_language; // Modify Language，0x10 You can modify the language of the device.

byte cmd\_version; // Instruction version

### Sample

int ret = CChex\_GetBasicConfigInfo(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.；

## CChex\_SetBasicConfigInfo

### Description functions

【Function】Set the basic configuration of the Anviz device

### Request

【Mode】int CChex\_SetBasicConfigInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_BASIC\_CFG\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；Unmodified fields，0xFF

uint password; // Password，String convert into number

byte pwd\_len; // Password length

byte delay\_for\_sleep; // Delay sleep time，0~250 Mins，0 don’t sleep

byte volume; // Volume，0~5，0：mute，5：Max

byte language; // Language，0：Simplified Chinese，1：Traditional Chinese，2：English，3.French，4：Spanish，5：Portuguese

byte date\_format; // Date format，0:Chinese，1：UK，2：USA

byte time\_format; // Time format，0：24Houes，1：12Hours

byte machine\_status; // Attendance Status，0~15

byte modify\_language; // Modify Language，0x10 You can modify the language of the device.

byte rsv; // Reserved

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetBasicConfigInfo(anviz\_handle, dev\_idx, ref set\_basic\_cfg);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_ListPersonInfo

### Description functions

【Function】Get all user information.

### Request

【Mode】int CChex\_ListPersonInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int CurIdx; // Current index number

int TotalCnt; // The total number of users

byte [5]EmployeeId; // User ID，5 bytes,Longest 12digits

byte password\_len; // Password length

byte max\_password; // Maximum length of password,= 6，unchangeable

int password; // Password

byte max\_card\_id; // The maximum length of the card number，= 6（3bytes）or 10 （4bytes）, unchangeable

uint card\_id; // Card number

byte max\_EmployeeName; // The maximum length of a user's name，= 10、20 、64 and160,unchangeable；=160 ,The user name is stored in EmployeeName2.

byte[64] EmployeeName; // User name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Attendance mode

uint Fp\_Status; // Fingerprint register status，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // Employee Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

### Sample

int ret = CChex\_ListPersonInfo(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_ModifyPersonInfo

### Description functions

【Function】Modify the relevant user’s information.

### Request

【Mode】int CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

person\_num，How many users were changed，Input[Parameter]；

Personlist，user details information，Input[Parameter]；

uint MachineId; // Device ID

int CurIdx; // Current index number

int TotalCnt; // The total number of users

byte [5]EmployeeId; // User ID，5 bytes,Longest 12digits

byte password\_len; // Password length

byte max\_password; // Maximum length of password,= 6，unchangeable

int password; // Password

byte max\_card\_id; // The maximum length of the card number，= 6（3bytes）or 10 （4bytes）, unchangeable

uint card\_id; // Card number

byte max\_EmployeeName; // The maximum length of a user's name，= 10、20 、64 and160,unchangeable；=160 ,The user name is stored in EmployeeName2.

byte[64] EmployeeName; // User name

byte DepartmentId; // Department ID

byte GroupId; // Group

byte Mode; // Attendance mode

uint Fp\_Status; // Fingerprint register status，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User name 2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_ModifyPersonInfo(anviz\_handle, dev\_idx, ref item, 1);

### Notice

1.Make sure that CChex\_Start has been started successfully before run；

## CChex\_DeletePersonInfo

### Description functions

【Function】Deletes the assigned person’s information.

### Request

【Mode】int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_PERSON\_INFO\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config,Input[Parameter]；

byte []EmployeeId; // User ID

byte operation; // Which information be deleted ? The 3 digits: Card; The 2 digits: Password; The 1~0 digits: 1~0 digits ：11; 7~4 digits：10 Fingerprints（1~10）；0xFF: Delete all user’s information .

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_DeletePersonInfo(anviz\_handle, dev\_idx, ref delete\_item);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_DeletePersonInfo\_VER\_4\_NEWID

### Description functions

【Function】Delete the user’s information

(Version:User ID for Chat DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)

### Request

【Mode】int CChex\_DeletePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_DEL\_EMPLOYEE\_INFO\_STRU\_EXT\_INF\_ID\_VER\_4\_NEWID Config);

【Parameter】CchexHandle：successfully create by CChex\_Start the handle，Input[Parameter]；；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte [28]EmployeeId; // User ID for the String

byte operation; // Delete user Information the 3 bit is card, The 2 bit is Password ,The 0~1 byte is 11 and the 7~14 bit is number of the fingerprints(1~10)； 0xFF，delete all user information

### Response

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_DEL\_EMPLOYEE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [28] EmployeeId; // User ID for the String

### Sample

int ret = CChex\_DeletePersonInfo(anviz\_handle, dev\_idx, ref delete\_item);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadFingerPrint

### Description functions

【Function】Download fingerprint template from Anviz device

### Request

【Mode】int CChex\_DownloadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx,Search the device，Input[Parameter]；

EmployeeId，User ID, Input[Parameter]；

FingerIdx，Fingerprint Indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte []EmployeeId; // User ID

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10

uint fp\_data\_len; // The length of the fingerprint data.

byte []Data; // fingerprint data

### Sample

int ret = CChex\_DownloadFingerPrint(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_DownloadFingerPrint\_VER\_4\_NEWID

### Function

【Function】Download the fingerprint information from the device

**(Version:device version DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### Request

【Mode】int CChex\_DownloadFingerPrint\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

EmployeeId: byte[28]User ID，Input[Parameter]; User ID for the String FingerIdx: Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

### Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_DLFINGERPRT\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte [28]EmployeeId; // User ID //User ID for the String ID byte[28]

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10

uint fp\_data\_len; // The length of the fingerprint data.

byte []Data; // fingerprint data

### Sample

int ret = CChex\_DownloadFingerPrint\_VER\_4\_NEWID(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_UploadFingerPrint

### Description functions

【Function】Upload fingerprint template to Anviz device

### Request

【Mode】int CChex\_UploadFingerPrint(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

EmployeeId，User ID，Input[Parameter]；

FingerId; Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

FingerData，fingerprint data，Input[Parameter]；

DataLen，The length of the fingerprint data，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_DownloadFingerPrint(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_UploadFingerPrint\_VER\_4\_NEWID

### Function

【Function】Upload the fingerprint template to device (Device Type:"FACEPASS7" For :FaceTemplate download )

**(Version:Device Version Model DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### Request

【Mode】int CChex\_UploadFingerPrint\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, byte[] EmployeeId, byte FingerIdx, byte[] FingerData, int DataLen);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；；

DevIdx: Index of device，Input[Parameter]；

EmployeeId: User ID，Input[Parameter]; //User ID for the String ID byte[28]

FingerIdx: Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

FingerData，fingerprint data，Input[Parameter]；

DataLen，The length of the fingerprint data，Input[Parameter]；

### Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_ULFINGERPRT\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte []EmployeeId; // /User ID for the String ID byte[28]

byte FpIdx; // Fingerprint indexing，1~10：means fingerprint number 1~10，Input[Parameter]；

uint fp\_data\_len; // The length of the fingerprint data

byte []Data; // Fingerprint Data

### Sample

int ret = CChex\_DownloadFingerPrint\_VER\_4\_NEWID(anviz\_handle, dev\_idx, EmployeeID, FpIdx);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetTime

### Description functions

【Function】Get the date/time of the Anviz device.

### Request

【Mode】int CChex\_GetTime(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_MSG\_GETTIME\_STRU Cfg;

uint Year; //Year

uint Month; //Month

uint Day; //Day

uint Hour; //Hour

uint Min; //Minute

uint Sec; //Second

### Sample

int ret = CChex\_GetTime(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_InitUserArea

### Description functions

【Function】Initial user area

Initialize all user data areas，Clear all user data, fingerprint data, password/card data.

### Request

【Mode】int CChex\_InitUserArea(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_InitUserArea(anviz\_handle, dev\_idx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_InitSystem

### Description functions

【Function】initial device

initialize the Anviz device to restore factory Default.

### Request

【Mode】int CChex\_InitSystem(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_InitSystem(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetBasicConfigInfo2

### Description functions

【Function】Get the Anviz device’s configuration2

Get device’s identification precision, fixed wiegand head, wiegand mode, workcode, real-time attendance records , schedule bell , lock control delay, record overflow warning, repeated attendance record time , door sensor delay, schedule bell delay.

### Request

【Mode】int CChex\_GetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF Param;

byte compare\_level; //identification precision

byte wiegand\_range; //fixed wiegand head

byte wiegand\_type; //wiegand mode

byte work\_code; //Workcode function, enable or disable?

byte real\_time\_send; //Realtime function ,enable or disable?

byte auto\_update; //Auto-update function, enable or disable?

byte bell\_lock; //Schedule bell function, enable or disable?

byte lock\_delay; //Lock time delay

uint record\_over\_alarm; //Record overflow alarm

byte re\_attendance\_delay; //Repeat attendance time delay

byte door\_sensor\_alarm; //Door sensor time delay

byte bell\_delay; //Schedule bell time delay

byte correct\_time; //Time calibration

### Sample

int ret = CChex\_GetBasicConfigInfo2(anviz\_handle, dev\_idx);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetBasicConfigInfo2

### Description functions

【Function】Set up the Anviz device’s configuration information2

### Request

【Mode】int CChex\_SetBasicConfigInfo2(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_BASIC\_CFG\_INFO2\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

config: Input[Parameter]；

byte compare\_level; //identification precision

byte wiegand\_range; //fixed wiegand head

byte wiegand\_type; //wiegand mode

byte work\_code; //Workcode function, enable or disable?

byte real\_time\_send; //Realtime function ,enable or disable?

byte auto\_update; //Auto-update function, enable or disable?

byte bell\_lock; //Schedule bell function, enable or disable?

byte lock\_delay; //Lock time delay

uint record\_over\_alarm; //Record overflow alarm

byte re\_attendance\_delay; //Repeat attendance time delay

byte door\_sensor\_alarm; //Door sensor time delay

byte bell\_delay; //Schedule bell time delay

byte correct\_time; //Time calibration

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetBasicConfigInfo2(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_GetPeriodTime

### Description functions

【Function】Get time zone from device

Read the timezone information，Total 32 timezones。

### Request

【Mode】int CChex\_GetPeriodTime(IntPtr CchexHandle, int DevIdx, byte SerialNumbe);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

SerialNumbe,timezone number，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day[7]; //One week 7 days,28Byte

byte StartHour; //Start hour

byte StartMin; //Start mins

byte EndHour; //End hour

byte EndMin; //End mins

### Sample

int ret = CChex\_GetPeriodTime(anviz\_handle, dev\_idx,SerialNumbe);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetPeriodTime

### Description functions

【Function】Set timezone

Total 32 timezones。

### Request

【Mode】int CChex\_SetPeriodTime(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_PERIOD\_TIME\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte SerialNumbe;

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day[7]; //one week with 7 days,so should be have 7 groups,28Byte

byte StartHour; //Start Hour

byte StartMin; //Start Mins

byte EndHour; //End Hours

byte EndMin; //End Mins

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetPeriodTime(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run；

## CChex\_GetTeamInfo

### Description functions

【Function】Get Group information

Read one group information, group number 0-16, group0 = normal close; group1=normal open. Only read group2 - group16.

### Request

【Mode】int CChex\_GetTeamInfo(IntPtr CchexHandle, int DevIdx, byte TeamNumbe);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

TeamNumbe:Group number,Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[4] PeriodTimeNumber;//4Group timezone number(refer to 2.29)

### Sample

int ret = CChex\_GetTeamInfo(anviz\_handle, dev\_idx,TeamNumbe);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CChex\_SetTeamInfo

### Description functions

【Function】Setup group

Setup one group, group number 0- 16, group 0= normal close; group1= normal open, only setup group2 -group16.

### Request

【Mode】int CChex\_SetTeamInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_TEAM\_INFO\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config: Input[Parameter]；

byte TeamNumbe; //Group Number

byte[4] PeriodTimeNumber; //4Group ,timezone

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CChex\_SetTeamInfo(anviz\_handle, dev\_idx,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_AddFingerprintOnline

### Description functions

【Function】Register fingerprint online

### Request

【Mode】int CCHex\_AddFingerprintOnline(IntPtr CchexHandle, int DevIdx, ref CCHEX\_ADD\_FINGERPRINT\_ONLINE\_STRU\_EXT\_INF Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: Input[Parameter]；

byte[5] EmployeeId; //User ID

byte BackupNum; //Backup number

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_AddFingerprintOnline(anviz\_handle, dev\_idx,ref Param);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.
2. After the recall, the device will register the fingerprint twice, timeout is 10 seconds, the registration error (timeout, operation failure, the user already exists, the fingerprint exists) returned -1, and successfully returns 0.

## CCHex\_ForcedUnlock

### Description functions

【Function】Open the door by software (Force open the lock)

### Request

【Mode】int CCHex\_ForcedUnlock(IntPtr CchexHandle, int DevIdx, ref CCHEX\_FORCED\_UNLOCK\_STRU\_EXT\_INF Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: Input[Parameter]；( Param =IntPtr.Zerohe ; default null pointer , Malaysia panasonic project customization needs to enter Param);

byte LockCmd; //Lock command

byte[5] EmployeeId; //User ID

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_ForcedUnlock(anviz\_handle, DevIdx,IntPtr.Zero);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.；
2. If Not Malaysia Panasonic project customization, Param none pointer..

## CCHex\_Udp\_Search\_Dev

### Description functions

【Function】UDP Research the Anviz device

### Request

【Mode】int CCHex\_Udp\_Search\_Dev(IntPtr CchexHandle);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：(Data length =sizeof(int)+DevNum\*sizeof(CCHEX\_UDP\_SEARCH\_STRU\_EXT\_INF))

int DevNum; // quantity of device, ( =0, No device,data length =4)

CCHEX\_UDP\_SEARCH\_STRU\_EXT\_INF[] dev\_net\_info ; //Device Data(Single 180Byte)

uint MachineId; //Device ID

int Result; //0: ok -1: fail

int DevHardwareType; //device type(0:Normal device;1:support DNS;2:support wifi)

byte[167] Data; //Data(Convert based on device type)

Byte Padding; //Data alignment, padding

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

byte[167] Data: Data type definition

Device type = 0 :Normal device

CCHEX\_UDP\_SEARCH\_STRU BasicSearchInfo; //normal device 63Byte

byte[10] DevType; //device type

byte[16] DevSerialNum; //device serial numebr

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //network mode

byte[8] Version; //Firmware version

byte[4] Reserved; //Reserved

Device type = 1 :Support DNS firmware

CCHEX\_UDP\_SEARCH\_WITH\_DNS\_STRU DnsSearchInfo; //Support DNS firmware 167Byte

CCHEX\_UDP\_SEARCH\_STRU BasicSearchInfo; //device type 0:normal device 63Byte structure

byte[4] Dns; //DNS

byte[100] Url; //URL

Device type = 2 : Support wifi

CCHEX\_UDP\_SEARCH\_TWO\_CARD\_STRU TwocardSearchInfo; \\ support wifi 102Byte

byte[10] DevType; //Device type

byte[16] DevSerialNum; //Device serial number

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //Network mode

byte[8] Version; //Firmware version

byte[4] Reserved; //Reserved

byte CardNumber; //Network card number

CCHEX\_UDP\_SEARCH\_CARD\_STRU CardInfo[2]; //2group network card information: single network card information = 28Byte

byte[10] CardName; //Network card name

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC Address

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

### Sample

int ret = CCHex\_Udp\_Search\_Dev(anviz\_handle);

### Notice

1. Make sure that CChex\_Start has been started successfully before run.

## CCHex\_Udp\_Set\_Dev\_Config

### Description functions

【Function】UDP setting device configuration

### Request

【Mode】int CCHex\_Udp\_Set\_Dev\_Config(IntPtr CchexHandle, ref CCHEX\_UDP\_SET\_DEV\_CONFIG\_STRU\_EXT\_INF config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

Config: Input[Parameter]；

byte[4] IpAddr; //IP Address

byte[4] IpMask; //MASK

byte[4] GwAddr; //Gateway

byte[6] MacAddr; //MAC address

byte[4] ServAddr; //Server IP

byte[2] Port; //Port

byte NetMode; //Network mode

byte[3] Padding; //structure alignment,padding 3byte

uint NewMachineId; //New Device ID

byte[4] Reserved; //Reserved

byte[12] DevUserName; //User name

byte[12] DevPassWord; //Password

int DevHardwareType; //Device type 0:Normal device ;1:support DNS device

byte[4] Dns; //DNS device type = 0 Dns , unchangeable

byte[100] Url; //URL device type = 0 Url,unchangeable

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### Sample

int ret = CCHex\_Udp\_Set\_Dev\_Config(anviz\_handle,ref config);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_ClientConnect

### Description functions

【Function】The client actively connects to the server.

### Request

【Mode】int CCHex\_ClientConnect(IntPtr CchexHandle, byte[] Ip, int Port);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

Ip: Server IP address，Input[Parameter]；

Port: Server Port, Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】Failure:CChex\_Update,Type return CCHEX\_RET\_CLINECT\_CONNECT\_TYPE;

Data Part：

int Result; //-1 err

byte[24] Addr; //IP:Port 如(192.168.100.100:5010)

Successful:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int DevIdx; //

uint MachineId; //Device ID

byte[24] Addr; //IP:Port For example(192.168.100.100:5010)

byte[8] Version; //Version Number

byte[8] DevType; //Device type

int DevTypeFlag; //Type flag

### Sample

int ret = CCHex\_ClientConnect(anviz\_handle,Ip,Port);

### Notice

1. 1.Make sure that CChex\_Start has been started successfully before run.

## CCHex\_ClientDisconnect

### Description functions

【Function】The client actively disconnects the server.

### Request

【Mode】int CCHex\_ClientDisconnect(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】Failure:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int Result; // -1:error

int DevIdx; //

Successful:CChex\_Update, Type return CCHEX\_RET\_MSGADDNEW\_UNICODE\_INFO\_TYPE

Data Part：

int DevIdx; //Index of device，Input[Parameter]；

uint MachineId; //Device ID

uint Live; //

byte[24] Addr; //ip:Port 如(192.168.100.100:5010)

byte[8] Version; //Version number

byte[8] DevType; //Device type

### Sample

int ret = CCHex\_ClientDisconnect(anviz\_handle,DevIdx);

### Notice

1.Make sure that CChex\_Start has been started successfully before run.

## 2.42 CChex\_GetInfomationCode

### 2.42.1 Description function

【Function】Gets the factory information

Read the factory information ANSI version data:10Byte,UNICODE version data:20Byte

### 2.42.2 Request

【Mode】int CChex\_GetInfomationCode(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.40.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_INFOMATION\_CODE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int fp\_len; //ANSI VERSION:fp\_len == 10 UNICODE VERSION:fp\_len == 20

byte[20] data; //

### 2.42.4 Sample

int ret = CChex\_GetInfomationCode(anviz\_handle, dev\_idx);

### 2.42.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.43 CChex\_SetInfomationCode

### 2.43.1 Description function

【Function】Modify the factory information

Modify the factory information ANSI version data:10Byte ,UNICODE version data:20Byte

### 2.43.2 Request

【Mode】int CChex\_SetInfomationCode(IntPtr CchexHandle, int DevIdx ,byte[] Data, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data: Byte[10] or Byte[20] parameter，Input[Parameter]；

DataLen: Write the parameters based on the version, , ANSI version = 10,UNICODE version = 20, Input[Parameter]；

### 2.43.3Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_INFOMATION\_CODE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.43.4 Sample

int ret = CChex\_SetInfomationCode(anviz\_handle, dev\_idx,Data,DataLen);

### 2.43.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.44 CChex\_GetBellInfo

### 2.44.1 Description function

【Function】Get the Schedule bell information

Read all time of schedule bell，totally 30.

### 2.44.2 Request

【Mode】int CChex\_GetBellInfo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.44.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_BELL\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_RET\_GET\_BELL\_TIME\_POINT time\_point[30];

byte hour;

byte minute;

byte flag\_week; //Week mark/flag(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

Byte[2] padding; //data structure alignment , invalid data

### 2.44.4 Sample

int ret = CChex\_GetBellInfo(anviz\_handle, dev\_idx);

### 2.44.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.45 CChex\_SetBellInfo

### 2.45.1 Description function

【Function】Setup the schedule bell information

Setup the time of schedule bell

### 2.45.2 Request

【Mode】int CChex\_SetBellInfo(IntPtr CchexHandle, int DevIdx ,byte BellTimeNum,byte Hour,byte Min,byte FlagWeek);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

BellTimeNum：The time to ring the bell，Input[Parameter]；

Hour：Hour，Input[Parameter]；

Min：Minute，Input[Parameter]；

FlagWeek：Week mark/flag(Binary 0000000means：Sat Fri Thu Wed Tue Mon Sun)，Input[Parameter]；

### 2.45.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_BELL\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.45.4 Sample

int ret = CChex\_SetBellInfo(CchexHandle,DevIdx ,BellTimeNum,Hour,Min,FlagWeek);

### 2.45.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.46 CChex\_GetUserAttendanceStatusInfo

### 2.46.1 Description function

【Function】Gets the self-defining attendance status table

Read the information of self-defining attendance status.

### 2.46.2 Request

【Mode】int CChex\_GetUserAttendanceStatusInfo(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.46.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_USER\_ATTENDANCE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int fp\_len; //ANSI VERSION：fp\_len == 80 UNICODE VERSION fp\_len == 160

Byte atten\_status\_number; //Number of attendance status == 8 default

Byte[160] data\_info; //data format: ANSI VERSION: unsigned char [8][10] UNICODE VERSION: unsigned char[8][20] 。

Byte[3] padding; //data structure alignment, invalid data

### 2.46.4 Sample

int ret = CChex\_GetUserAttendanceStatusInfo(anviz\_handle, dev\_idx);

### 2.46.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.47 CChex\_SetUserAttendanceStatusInfo

### 2.47.1 Description function

【Function】Setup the self-defining attendance status

Setup the self-defining attendance status.

### 2.47.2 Request

【Mode】int CChex\_SetUserAttendanceStatusInfo(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_USER\_ATTENDANCE\_STATUS\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：8 groups self-defining status,Input[Parameter]；

uint fp\_len;//ANSI VERSION fp\_len = 80 UNICODE VERSION fp\_len = 160

Byte atten\_status\_number; //Number of attendance status 8 default

Byte[160] data\_info;//ANSI VERSION:8][10]，UNICODE VERSION:[8][20]

Byte[3] padding; //alignment, invalid data

### 2.47.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_USER\_ATTENDANCE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.47.4 Sample

int ret = CChex\_SetUserAttendanceStatusInfo(CchexHandle,DevIdx ,ref Param);

### 2.47.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.48 CChex\_ClearAdministratFlag

### 2.48.1 Description function

【Function】Clear the administrator flag

Clear all administrator flag.

### 2.48.2 Request

【Mode】int CChex\_ClearAdministratFlag(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.48.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_CLEAR\_ADMINISTRAT\_FLAG\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.48.4 Sample

int ret = CChex\_ClearAdministratFlag(anviz\_handle, dev\_idx);

### 2.48.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.49 CChex\_GetSpecialStatus

### 2.49.1 Description function

【Function】Get the special status

Get the current special status. Only for VF30/VP30/T60+

### 2.49.2 Request

【Mode】int CChex\_GetSpecialStatus(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.49.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_SPECIAL\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte status; //Byte1：Door alarm status 0-normal ,status 1-alarm status; Byte5：Door status 0-close , 1-open; Byte6：Door sensor status 0-close, 1-open; Byte7：Lock status 0-close, 1-open

Byte[7] reserved; //reserved useless in the temporary

### 2.49.4 Sample

int ret = CChex\_GetSpecialStatus(anviz\_handle, dev\_idx);

### 2.49.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.50 CChex\_GetAdminCardnumberPassword

### 2.50.1 Description function

【Function】Read administrator card number or password. Only for T5/M5/T50m

Get administrator card number or password.

### 2.50.2 Request

【Mode】int CChex\_GetAdminCardnumberPassword(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.50.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_ADMIN\_CARD\_PWD\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte[13] data; //device type : T5A,T50

\* Parameter :data[13] : if the device type is T5A，so:

DATA Add card ;delete card ;stress/duress card; special information Byte 1-4 5-8 9-12 13

The special information define as below:

Byte 0：Add card

Byte 1：Delete card

Byte 2：Stress/duress

If the device type is T50，so:

DATA Password length+ passwod Reserved

Byte 1-3 4-13

Password length = Byte(1) >> 4

Byte[3] padding; //data structure alignment, invalid data

### 2.50.4 Sample

int ret = CChex\_GetAdminCardnumberPassword(anviz\_handle, dev\_idx);

### 2.50.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.51 CChex\_SetAdminCardnumberPassword

### 2.51.1 Description function

【Function】Setup administrator card or password. Only for T5/M5/T50M

Setup T5A/M5A admin card and T50M admin password.

### 2.51.2 Request

【Mode】int CChex\_SetAdminCardnumberPassword(IntPtr CchexHandle, int DevIdx,byte[] Data, int DataLen);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Data[13]：Parameter refer to 2.47 :data[13] description ，Input[Parameter]；

DataLen： length = 13，Input[Parameter]；

### 2.51.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_ADMIN\_CARD\_PWD\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.51.4 Sample

int ret = CChex\_SetAdminCardnumberPassword(CchexHandle,DevIdx,Data,DataLen);

### 2.51.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.52 CChex\_GetDSTParam

### 2.52.1 Description function

【Function】Read the daylight saving time parameters

Read the flag of daylight saving time and time zone .

### 2.52.2Request

【Mode】int CChex\_GetDSTParam(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.52.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_DST\_PARAM\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCCHEX\_SET\_DST\_PARAM\_STRU param; //16byte

byte enabled; //0-Disable 1-enable；

byte ate\_week\_type; //1-Date format 2-week format；

GET\_DST\_PARAM\_TIME start\_time; //7 byte

byte month;

byte day;

byte week\_num; //Weekly definition：0x01-0x04： First 1-4 week 0x81-0x82：Last1-2 week

byte flag\_week; //Week flag: flag\_week 0-6:(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

byte hour;

byte minute;

byte sec;

GET\_DST\_PARAM\_TIME special\_time； //7 byte

### 2.52.4 Sample

int ret = CChex\_GetDSTParam(anviz\_handle, dev\_idx);

### 2.52.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.53 CChex\_SetDSTParam

### 2.53.1 Description function

【Function】Setup daylight saving time

Setup daylight saving time flag and time zone

### 2.53.2 Request

【Mode】int CChex\_SetDSTParam(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DST\_PARAM\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：16byte，Input[Parameter]；

byte enabled; //0-disable 1-enable；

byte ate\_week\_type; //1-Date format 2-week format；

GET\_DST\_PARAM\_TIME start\_time; //7 byte

byte month;

byte day;

byte week\_num; //Weekly definition：0x01-0x04： First 1-4 week 0x81-0x82：Last1-2 week

byte flag\_week; //Week flag: flag\_week 0-6:(Binary 0000000 means：Sat Fri Thu Wed Tue Mon Sun)

byte hour;

byte minute;

byte sec;

GET\_DST\_PARAM\_TIME special\_time； //7 byte

### 2.53.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_DST\_PARAM\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.53.4 Sample

int ret = CChex\_SetDSTParam(CchexHandle,DevIdx,ref Param);

### 2.53.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.54 CChex\_GetDevExtInfo

### 2.54.1 Description function

【Function】Gets the device extension information code

Read the factory name/Tax number/factory Address

### 2.54.2 Request

【Mode】int CChex\_GetDevExtInfo(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.54.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_DEV\_EXT\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_SET\_DEV\_EXT\_INFO\_STRU param; //320byte

Byte[50] manufacturer\_name; //Factory name

Byte[100] manufacturer\_addr; //Address

Byte[15] duty\_paragraph; //Tax number

Byte[155] reserved; //Reserved

### 2.54.4 Sample

int ret = CChex\_GetDevExtInfo(CchexHandle,DevIdx);

### 2.54.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.55 CChex\_SetDevExtInfo

### 2.55.1 Description function

【Function】Modify the device extension information code

Modify the factory name/Tax number/factory Address

### 2.55.2 Request

【Mode】int CChex\_SetDevExtInfo(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DEV\_EXT\_INFO\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：320byte，Input[Parameter]；

Byte[50] manufacturer\_name; //factory name

Byte[100] manufacturer\_addr; //factory address

Byte[15] duty\_paragraph; //Tax number

Byte[155] reserved; //Reserved

### 2.55.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_DEV\_EXT\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.55.4 Sample

int ret = CChex\_SetDevExtInfo(CchexHandle,DevIdx,ref Param);

### 2.55.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.56 CChex\_GetBasicConfigInfo3

### 2.56.1Description function

【Function】Get the device configuration information3

Read Wiegand mode。

### 2.56.2 Request

【Mode】int CChex\_GetBasicConfigInfo3(IntPtr CchexHandle,int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.56.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_BASIC\_CFG3\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

CCHEX\_SET\_BASIC\_CFG\_INFO3\_STRU param; //15 byte

Byte wiegand\_type; //wiegand mode

Byte online\_mode; //online mode

Byte collect\_level; //Acquisition threshold

Byte pwd\_status; //communication password status =0 ,connect don’t need the communication password by TCP/IP; communication password status =1, send 0x04 command, verify the communication password by TCP/IP

Byte sensor\_status; //=0 don’t report the door sensor status; =1 activate report the door sensor status（the device will activate send the response of 0x2F command )

Byte[8] reserved; //Reserved

Byte independent\_time; //User independent time limit

Byte m5\_t5\_status; //= 0 disable; = 1 enable; Out =2, disable In =4 disable，out =5 disable，In

Byte padding; //alignment invalid data

### 2.56.4 Sample

int ret = CChex\_GetBasicConfigInfo3(CchexHandle,DevIdx);

### 2.56.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.57 CChex\_SetBasicConfigInfo3

### 2.57.1 Description function

【Function】Setup the device configuration information3

Read Wiegand mode

### 2.57.2 Request

【Mode】int CChex\_SetBasicConfigInfo3(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_BASIC\_CFG\_INFO3\_STRU Config);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Config：15byte，Input[Parameter]；

Byte wiegand\_type; //wiegand mode

Byte online\_mode; //Online mode

Byte collect\_level; //Acquisition threshold

Byte pwd\_status; //communication password status =0 ,connect don’t need the communication password by TCP/IP; communication password status =1, send 0x04 command, verify the communication password by TCP/IP

Byte sensor\_status; //=0 don’t report the door sensor status; =1 activate report the door sensor status（the device will activate send the response of 0x2F command )

Byte[8] reserved; //Reserved

Byte independent\_time; //User independent time limit

Byte m5\_t5\_status; //= 0 disable; = 1 enable; Out =2, disable In =4 disable，out =5 disable，In

### 2.57.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_SET\_BASIC\_CFG3\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.57.4 Sample

int ret = CChex\_SetBasicConfigInfo3(CchexHandle,DevIdx,ref Config);

### 2.57.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.58 CChex\_ConnectionAuthentication

### 2.58.1 Description function

【Function】connection identification

connection identification, identification successful, then response the other command; if the identification successful and no data transfer in 5 mins , recover to dis-identification mode

### 2.58.2 Request

【Mode】int CChex\_ConnectionAuthentication(IntPtr CchexHandle, int DevIdx,ref CCHEX\_CONNECTION\_AUTHENTICATION\_STRU Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：24byte，Input[Parameter]；

Byte[12] username;

Byte[12] password;

//Iris user name “admin”，password “admin”，

//Other devices, don’t identify user name, only identify communication password.

### 2.58.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_CONNECTION\_AUTHENTICATION\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.58.4 Sample

int ret = CChex\_ConnectionAuthentication(CchexHandle,DevIdx,ref Param);

### 2.58.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.59 CChex\_GetRecordNumByEmployeeIdAndTime

### 2.59.1 Description function

【Function】Get the record quantity by user ID and time. Only support A20/972 hardware platform devices.

Get the record quantity by user ID and time.

### 2.59.2 Request

【Mode】int CChex\_GetRecordNumByEmployeeIdAndTime(IntPtr CchexHandle, int DevIdx,ref CCHEX\_GET\_RECORD\_INFO\_BY\_TIME Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：13byte，Input[Parameter]；

Byte[5] EmployeeId; //User ID

Byte[4] start\_date; //The number of seconds after 2000.1.2 Byte[4] end\_date; //The number of seconds after 2000.1.2

User ID = 0xFF means all users

Start date = 0xFF, means unlimit the start date

End date = 0xFF, means unlimit the end date

### 2.59.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_NUMBER\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

int record\_num; // record quantity

### 2.59.4 Sample

int ret = CChex\_GetRecordNumByEmployeeIdAndTime(CchexHandle,DevIdx,ref Param);

### 2.59.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.60 CChex\_DownloadRecordByEmployeeIdAndTime

### 2.60.1 Description function

【Function】Get the record by user ID and time. Only support A20/972 hardware platform devices.

Get the record by user ID and time。

### 2.60.2 Request

【Mode】int CChex\_DownloadRecordByEmployeeIdAndTime(IntPtr CchexHandle, int DevIdx,ref CCHEX\_GET\_RECORD\_INFO\_BY\_TIME Param);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param：13byte，Input[Parameter]；

Byte[12] EmployeeId; //user ID

Byte[4] start\_date; //The number of seconds after 2000.1.2

Byte[4] end\_date; //The number of seconds after 2000.1.2

User ID = 0xFF means all users

Start date = 0xFF, means unlimit the start date

End date = 0xFF, means unlimit the end date

### 2.60.3Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_BY\_EMPLOYEE\_TIME\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

Byte[5] EmployeeId; //User ID

Byte[4] char date; //date time

Byte char back\_id; //back ID

Byte ecord\_type; //record type

Byte[3] work\_type; //work code

Byte[2] padding; //alignment invalid data

Note: The number of times this type of data is returned based on the number of records recorded during the output download time

### 2.60.4 Sample

int ret = CChex\_DownloadRecordByEmployeeIdAndTime(CchexHandle,DevIdx,ref Param);

### 2.60.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.61 Send attendance records in real time

### 2.61.1 Description function

【Function】Send the records in real time

After verification, the attendance information will be output automatically, and only the response information will be available.

### 2.61.2 Request

【Mode】

【Parameter】

### 2.61.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_LIVE\_SEND\_ATTENDANCE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

byte[5] EmployeeId; //user ID

byte[4] timestamp; //The number of seconds after 2000.1.2

Byte backup; //backup ID

byte record\_type; //record type

byte[3] work\_type[3]; //workcode

byte[2] padding[2];

### 2.61.4Sample

### 2.61.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

2. Set whether the device configuration information 2 is sent in real time

## 2.62 CChex\_GetRecordInfo

### 2.62.1 Description function

【Function】Get the record information

Get the record information, contains already register user quantity, already register FP quantity, already register password quantity, all record quantity and new record quantity

### 2.62.2 Request

【Mode】int CChex\_GetRecordInfoStatus(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.62.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_RECORD\_INFO\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

uint EmployeeNum; //User quantity

uint FingerPrtNum; //FP quantity

uint PasswdNum;

uint CardNum;

uint TotalRecNum;

uint NewRecNum;

### 2.62.4 Sample

int ret = CChex\_GetRecordInfoStatus(CchexHandle,DevIdx);

### 2.62.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.63 CChex\_DownloadAllNewRecords

### 2.63.1 Description function

【Function】Download all record

### 2.63.2Request

【Mode】int CChex\_DownloadAllNewRecords(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.63.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return CCHEX\_RET\_GET\_NEW\_RECORD\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

byte NewRecordFlag; // new record or no

byte[5] EmployeeId; // User ID，

byte[4] Date; // Time，The number of seconds after 2000.1.2

byte BackId; // Backup ID，3 digits：Card，2 digits：，1~0：11，digits 7~4：10 FP templates（1~10）

byte RecordType // Record type，7 digits：1：open the door，0：can’t open the door；3~0 digits attendance status

byte[3] WorkType; // workcode

byte Rsv // reserved

### 2.63.4 Sample

int ret = CChex\_DownloadAllNewRecords(anviz\_handle, dev\_idx);

### 2.63.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.64 Upload user information

【Function】upload user information

### 2.64.2 Request

【Mode】call the universal interface **2.20**  CChex\_ModifyPersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_RET\_PERSON\_INFO\_STRU personlist, byte person\_num);

**Call by the device type：dev->DevTypeFlag & 0xff**

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE\_INFO\_STRU EmployeeList, byte EmployeeNum);

ASCII universal：dev->DevTypeFlag & 0xff == 0x02

CChex\_UploadEmployee2Info(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2\_INFO\_STRU

EmployeeList, byte EmployeeNum);

UNICODE universal：dev->DevTypeFlag & 0xff == 0x04

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU

EmployeeList, byte EmployeeNum);

UNICODE\_W2 universal：dev->DevTypeFlag & 0xff == 0x20

CChex\_UploadEmployeeInfo(IntPtr \*CchexHandle, int DevIdx, ref CCHEX\_EMPLOYEE2W2\_INFO\_STRU

EmployeeList, byte EmployeeNum);

【Parameter】CchexHandle：,successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

EmployeeNum：Increase the number of employees (8 or 12 per upload per device type and customization)

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CCHEX\_EMPLOYEE\_INFO\_STRU //28byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //password

byte[3] CardId; //card ID

byte[10] EmployeeName; //name

byte DepartmentId; //department ID

byte GroupId; //Group ID

byte Mode; //Attendance mode

byte[2] FpStatus; //FP registration status

byte Special; //Count of the in formations

byte Padding; //Invalid structure alignment

ASCII Universal：dev->DevTypeFlag & 0xff == 0x02

CCHEX\_EMPLOYEE2\_INFO\_STRU //32byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[10] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

Byte[2] Padding; //Invalid structure alignment

UNICODE Universal：dev->DevTypeFlag & 0xff == 0x04

CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU //40byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[20] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //Password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

UNICODE\_W2 Universal：dev->DevTypeFlag & 0xff == 0x20

CCHEX\_EMPLOYEE2W2\_INFO\_STRU

CCHEX\_EMPLOYEE2UNICODE\_INFO\_STRU //40byte

byte[5] EmployeeId; //user id only one mark

byte[3] Passwd; //Password

byte[4] CardId; //Card Number

byte[20] EmployeeName; //Name

byte DepartmentId; //Department ID

byte GroupId; //Group ID

byte Mode; //Time attendance mode

byte[2] FpStatus; //Fingerprint Status

byte PwdH8bit; //Password high 8 bits

byte Rserved; //Save

byte Special; //Count of the in formations

byte[4] start\_date //Employee starting time，The number of seconds after 2000.1.2

byte[4] end\_date //Employee ending time，The number of seconds after 2000.1.2

### 2.64.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update, Type return

Universal 1：dev->DevTypeFlag & 0xff == 0x01

CCHEX\_RET\_ULEMPLOYEE\_INFO\_TYPE

ASCII Universal ：dev->DevTypeFlag & 0xff == 0x02

CCHEX\_RET\_ULEMPLOYEE2\_INFO\_TYPE

UNICODE Universal：dev->DevTypeFlag & 0xff == 0x04

CCHEX\_RET\_ULEMPLOYEE2UNICODE\_INFO\_TYPE

UNICODE\_W2 Universal：dev->DevTypeFlag & 0xff == 0x20

CCHEX\_RET\_ULEMPLOYEE2W2\_INFO\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:OK, -1:error

### 2.64.4 Sample

int ret = CChex\_UploadEmployeeInfo(anviz\_handle, dev\_idx，EmployeeList，1);

### 2.64.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.；

## 2.65 Chex\_GetBasicConfigInfo5

### 2.65.1 Function

【Function】获取考勤机配置信息5（Bolid定制）

### 2.65.2 Request

【Mode】int CChex\_GetBasicConfigInfo5(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；参；

### 2.65.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_BASIC\_CFG5\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

byte fail\_alarm\_time; // 勤失败报警次数: 0: 不报警1~10 N次失败报警

byte tamper\_alarm; // 防拆报警: 0: 关闭1: 开启

byte[94] reserved; // reserved

### 2.65.4 Sample

int ret = CChex\_GetBasicConfigInfo5(anviz\_handle, dev\_idx);

### 2.65.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.66 CChex\_SetBasicConfigInfo 5

### 2.66.1 Function

【Function】Setup Time attendance device information 5（Bolid Customize）

### 2.66.2 Request

【Mode】int CChex\_SetBasicConfigInfo5(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_BASIC\_CFG\_INFO5\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: //96 byte （0xFF means do not setup）

byte fail\_alarm\_time; // Times of Attendance Fail Alarm: 0: Do not alarm out 1~10 times of alarm out

byte tamper\_alarm; // Tamper alarm: 0: Close1: Active

byte[94] reserved; // reserved

### 2.66.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_BASIC\_CFG5\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

### 2.66.4 Sample

int ret = CChex\_SetBasicConfigInfo5(anviz\_handle, dev\_idx,ref Param);

### 2.66.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

Function

## 2.67 CChex\_GetCardNo

### 2.67.1 Function

【Function】Query T5S swipe card information（Bolid Customize）

**Notice**： 1：The first time call the function ：Setting the device as swipe card mode

2：Swipe card over time > 5sec；

3：The second time call the function ：Return the last Card number before called the function.

### 2.67.2 Request

【Mode】int Chex\_GetCardNo(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.67.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_CARD\_ID\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Uint card\_id; //Card Number

### 2.67.4 Sample

int ret = Chex\_GetCardNo(anviz\_handle, dev\_idx);

### 2.67.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.68 CChex\_SetDevCurrentStatus

### 2.68.1 Function

【Function】User to modify the device status by temporary（Bolid Customize）

### 2.68.2 Request

【Mode】int CChex\_SetDevCurrentStatus(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_DEV\_CURRENT\_STATUS\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param: //96 byte （0xFF means do not setup）

byte alarm\_stop; //Disable the Alarm except 0XFF

byte door\_status //0: Setting the access control as normal 1: Setting the access control as normal Open 2: Setting the access control as normal Close

byte[94] reserved; // reserved

### 2.68.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_DEV\_CURRENT\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

### 2.68.4 Sample

int ret = CChex\_SetDevCurrentStatus(anviz\_handle, dev\_idx,ref Param);

### 2.68.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.69 CChex\_GetServiceURL

### 2.69.1 Function

【Function】Get the server’s URL

### 2.69.2 Request

【Mode】int CChex\_GetServiceURL(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.69.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update return CCHEX\_RET\_GET\_URL\_TYPE

Data Part：

uint MachineId; // device ID

Int Result; // 0:Success -1：Fail

Byte[4] Dns //dns address

byte[100] Url; //URL address

### 2.69.4 Sample

int ret = CChex\_GetServiceURL(anviz\_handle, dev\_idx);

### 2.69.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.70 CChex\_SetServiceURL

### 2.70.1 Function

【Function】Setuphe server’s URL

### 2.70.2 Request

【Mode】int CChex\_SetServiceURL(IntPtr CchexHandle, int DevIdx,ref CCHEX\_SET\_URL\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param: //104 byte

Byte[4] Dns //dns Address

byte[100] Url; //URL Address

### 2.70.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_SET\_URL\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Success -1：Fail

### 2.70.4 Sample

int ret = CChex\_SetServiceURL(anviz\_handle, dev\_idx,ref Param);

### 2.70.15 Notice

1.Make sure the CChex\_Start already active before running

## 2.71 CChex\_UploadFile

### 2.71.1 Function

【Function】Update firmware, Image and Voice

### 2.71.2 Request

【Mode】int CChex\_UploadFile(IntPtr CchexHandle, int DevIdx, byte FileType, byte[] FileName, byte[] Buff, int Len);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

FileType: = 0 Firmware，= 1 Image，= 2 Voice，= 3 Language

FileName: The name update to the device（MAX\_len = 10)；

Buff: The uploaded file is read as a string;

Len： The length of the string of the uploaded file.

### 2.71.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_UPLOADFILE\_TYPE

Data Part：

uint MachineId; // Device ID

int Result; // 0:Success -1：Fail

uint TotalBytes; // Total length of the uploaded string

uint SendBytes; // Length already uploaded

**Notice：Every 32K of data is uploaded will return the type once SendBytes == TotalBytes，the upload is completed.**

### 2.71.4 Sample

int ret = CChex\_UploadFile(CchexHandle,DevIdx,FileType,FileName,Buff,Len);

### 2.71.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.72 CChex\_UpdateDevStatus

### 2.72.1 Function

【Function】ask device the status of the firmware updating

**Notice:** After the upgrade package is uploaded, it is called multiple times. When the result is: 1: Check completion 2: The verification is successful. You can restart the upgrade

### 2.72.2 Request

【Mode】int CChex\_UpdateDevStatus(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

### 2.72.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_UPDATEFILE\_STATUS\_TYPE

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Success -1：Fail

int verify\_status; // 0:verifying ;1: Verify Success

int verify\_ret; // 0:Verify Success;1: Verify Fail

### 2.72.4 Sample

int ret = CChex\_UpdateDevStatus(anviz\_handle, dev\_idx);

### 2.72.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.73 CChex\_GetStatusSwitch

### 2.73.1 Function

【Function】Get status switch information, total with 16 status

**Notice：Device TypeDevTypeFlag & 0x200000 = = 1 can be called**

### 2.73.2 Request

【Mode】int CChex\_GetStatusSwitch(IntPtr CchexHandle, int DevIdx,byte GroupId);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

GroupId：Edit Group ID

### 2.73.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_STATUS\_SWITCH\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

byte group\_id; //get the group number

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day\_week[7]; //7 groups as 7day for one week. One group with 28Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[2] padding; //Invalid data, fill in the structure

### 2.73.4 Sample

int ret = CChex\_GetStatusSwitch(anviz\_handle, dev\_idx,GroupId);

### 2.73.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.74 CChex\_SetStatusSwitch

### 2.74.1 Function

【Function】Setup status switch information, total with 16 status

**Notice：Device Type DevTypeFlag & 0x200000 = = 1 can be called**

### 2.74.2 Request

【Mode】int CChex\_SetStatusSwitch(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_STATUS\_SWITCH\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param： // 32 byte

byte group\_id; //get the group number

CCHEX\_GET\_PERIOD\_TIME\_ONE\_STRU\_EXT\_INF day\_week[7]; // 7 groups as 7day for one week. One group with 28Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[2] padding; //Invalid data, fill in the structure

### 2.74.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_STATUS\_SWITCH\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

### 2.74.4 Sample

int ret = CChex\_SetStatusSwitch(anviz\_handle, dev\_idx,ref Param);

### 2.74.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.75 CChex\_GetStatusSwitch\_EXT

### 2.75.1 Function

【Function】Get status switch information

**Notice：Device TypeDev TypeFlag & 0x100000 = = 1 can be called**

### 2.75.2 Request

【Mode】int CChex\_GetStatusSwitch\_ext(IntPtr CchexHandle, int DevIdx,byte FlagWeek);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

FlagWeek：Week day as 0-6，to represent Sun. to Sat., Such as Monday ：00000010

### 2.75.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_GET\_STATUS\_SWITCH\_EXT\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

byte flag\_week; //get the group number

CCHEX\_ONE\_TIMER\_STATUS one\_time[8]; //8 time zone 40Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[3] padding; //Invalid data, fill in the structure

### 2.75.4 Sample

int ret = CChex\_GetStatusSwitch\_EXT(anviz\_handle, dev\_idx,flag\_week);

### 2.75.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.76 CChex\_SetStatusSwitch\_EXT

### 2.76.1 Function

【Function】Setup time attendance status information

**Notic：Device type DevTypeFlag & 0x100000 = = 1 can be call**

### 2.76.2 Request

【Mode】int CChex\_SetStatusSwitch\_EXT(IntPtr CchexHandle, int DevIdx, ref CCHEX\_SET\_STATUS\_SWITCH\_STRU\_EXT Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Search the device，Input[Parameter]

Param： // 44 byte

byte flag\_week; //get the group number

CCHEX\_ONE\_TIMER\_STATUS one\_time[8]; //8 timezone 40Byte

byte StartHour; //Starting Hour

byte StartMin; //Starting Mins

byte EndHour; //Ending Hour

byte EndMin; //Ending Mins

byte status\_id; //Setup status number

Byte[3] padding; //Invalid data, fill in the structure

### 2.76.3 Response

【Return value】1：The command was executed successfully.；Minus：Execute command failure

【Actual Data】CChex\_Update Type return CCHEX\_RET\_SET\_STATUS\_SWITCH\_EXT\_TYPE

Data Part：

uint MachineId; // Device IDInt Result; // 0:Success -1：Fail

### 2.76.4 Sample

int ret = CChex\_SetStatusSwitch\_EXT(anviz\_handle, dev\_idx,ref Param);

### 2.76.5 Notice

1. Make sure the CChex\_Start already active before running

## 2.77 CChex\_Get\_Service\_Port

### 2.77.1 Function

【Function】Setup the current server port

### 2.77.2 Request

【Mode】int CChex\_Get\_Service\_Port(IntPtr CchexHandle);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

### 2.77.3 Sample

int ret = CChex\_Get\_Service\_Port(CchexHandle);

【Return value】Returnret as server port

## 2.78 CChex\_SetSdkConfig

### 2.78.1 Function

【Function】Monitor the records status, the new record will automatic download and after download new records automatic to make a flag and SDK will print out to the LOG folder.

\* after CChex\_Start();

\* para :

\* SetRecordflag = 1 set recordflag after download new record;else = 0

\* SetLogFile = 1 set some info log to file for find problem ;else = 0

\* if do not set "CChex\_SetSdkConfig(void \*CchexHandle,int SetAutoDownload,int SetRecordflag,int SetLogFile)", config is default

\* ANVIZ\_DEFAULT:

\* W2 : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

\* SEATS : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

\* DR : SetRecordflag = 0,SetLogFile = 0,SetAutodownload = 1;

\* COMMON : SetRecordflag = 0,SetLogFile = 0,SetAutodownload = 1;

\* Bolid : SetRecordflag = 1,SetLogFile = 0,SetAutodownload = 1;

### 2.78.2 Request

【Mode】void CChex\_SetSdkConfig(IntPtr CchexHandle, int SetAutoDownload,int SetRecordflag, int SetLogFile);

【Parameter】SetAutodownload: = 1: Monitor records status , when get new records automatic download record,others do not download automatic

SetRecordflag: = 1:After download new records automatic to make a flag.

SetLogFile: = 1:SDK Print out to Log file

### 2.78.3 Sample

int ret = CChex\_SetSdkConfig(CchexHandle,1,1,0);

;

## 2.79 CChex\_UploadRecord

### 2.79.1 Function

【Function】Upload Time Attendance Records

### 2.79.2 Request

【Mode】int CChex\_UploadRecord(IntPtr CchexHandle, int DevIdx, ref CCHEX\_UPLOAD\_RECORD\_INFO\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[5] EmployeeId; //Employee Id

Byte[4] char date; //Date

Byte char back\_id; //Backup ID

Byte ecord\_type; //Record Type

Byte[3] work\_type; //Work Code

### 2.79.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_UPLOAD\_RECORD\_TYPE //87

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Byte[5] EmployeeId; // digital of Employee Id

Byte[3] padding; // 无效数据结构对齐

### 2.79.4 Sample

int ret = CChex\_UploadRecord(anviz\_handle, dev\_idx,ref Param);

### 2.79.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.80 CChex\_UploadRecord\_VER\_4\_NEWID

### 2.80.1 Function

【Function】Upload Time Attendance Records

**(Version: Device Type DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### 2.80.2 Request

【Mode】int CChex\_UploadRecord\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, ref CCHEX\_UPLOAD\_RECORD\_INFO\_STRU\_VER\_4\_NEWID Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[28] EmployeeId; // String of Employee Id

Byte[4] date; //Date

Byte back\_id; //Backup ID

Byte ecord\_type; //Record Type

Byte[3] work\_type; //Work Code

### 2.80.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_UPLOAD\_RECORD\_TYPE //87

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

Byte[28] EmployeeId; // String of Employee Id

### 2.80.4 Sample

int ret = CChex\_UploadRecord\_VER\_4\_NEWID(anviz\_handle, dev\_idx,ref Param);

### 2.80.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.81 CChex\_GetOnePersonInfo

**(Version :digital of Employee Id )**

## CChex\_GetOnePersonInfo\_VER\_4\_NEWID

**(Version:**

**String of Employee Id DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

### 2.81.1 Function

【Function】According to employee Id to get user information

### 2.81.2 Request

【Mode】int CChex\_GetOnePersonInfo(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_ONE\_EMPLOYEE\_INFO\_STRU Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[5] EmployeeId; //digital of Employee Id

【Mode】int CChex\_GetOnePersonInfo\_VER\_4\_NEWID(IntPtr CchexHandle, int DevIdx, ref CCHEX\_GET\_ONE\_EMPLOYEE\_INFO\_STRU\_VER\_4\_NEWID Param);

**(Version :Device Version DevTypeFlag & 0XFF ==DEV\_TYPE\_VER\_4\_NEWID)**

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[28] EmployeeId; //String of Employee Id

### 2.81.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_ONE\_EMPLOYEE\_INFO\_TYPE //88

Data Part：

**digital of Employee Id ,Without employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [5]EmployeeId; // User ID 5 bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

**digital of Employee Id ,With employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [5]EmployeeId; // User ID 5 bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

byte[4] start\_date; // RFC Information

byte[4] end\_date; // CURP Information

**String of Employee Id , with employee valid time:**

uint MachineId; // Device ID

int CurIdx; // Current index ID

int TotalCnt; // Total number of User

byte [28]EmployeeId; // Enployee ID,28bytes

byte password\_len; // Length of the Password

byte max\_password; // Max length of the Password, the value is 6 Can not modify

int password; // Password

byte max\_card\_id; // Max length of the Card Number, the value is 6(3 byte) or 10(3 byte) Can not modify

uint card\_id; // Card Number

byte max\_EmployeeName; // Max length of the User Name, the value is 10,20,64 or 64(3 byte) When the value is 160 the user name store in the EmployeeName2

byte[64] EmployeeName; // User Name

byte DepartmentId; // Department ID

byte GroupId; // Group ID

byte Mode; // Time Attendance Mode

uint Fp\_Status; // The status of FP enroll，0~9:fp; 10:face; 11:iris1; 12:iris2

byte Rserved1; // for 22

byte Rserved2; // for 72 and 22

byte Special; // Special information

// DR info

byte[160] EmployeeName2; // User Name2

byte[13] RFC; // RFC Information

byte[18] CURP; // CURP Information

byte[4] start\_date; // RFC Information

byte[4] end\_date; // CURP Information

### 2.81.4 Sample

int ret = CChex\_UploadRecord(anviz\_handle, dev\_idx,ref Param);

int ret = CChex\_UploadRecord\_VER\_4\_NEWID(anviz\_handle, dev\_idx,ref Param);

### 2.81.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.82 CChex\_GetMachineId

### 2.82.1 Function

【Function】Read the device communication device ID

### 2.82.2 Request

【Mode】int CChex\_GetMachineId(IntPtr CchexHandle, int DevIdx);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

### 2.82.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_GET\_MACHINE\_ID\_TYPE //84

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

uint cur\_machineid; //Communicatrion device ID

### 2.82.4 Sample

int ret = CChex\_GetMachineId(anviz\_handle, dev\_idx);

### 2.82.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.83 CChex\_SetMachineId

### 2.83.1 Function

【Function】Setting device Communication device ID

### 2.83.2 Request

【Mode】int CChex\_SetMachineId(IntPtr CchexHandle, int DevIdx,uint MachineId);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

MachineId: device Communication device ID;

### 2.83.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_SET\_MACHINE\_ID\_TYPE //85

Data Part：

uint MachineId; // Device ID

Int Result; // 0:Succes -1：Failure

uint cur\_machineid; //New Communicatrion device ID

uint old\_machineid; //Old Communicatrion device ID

### 2.83.4 Sample

int ret = CChex\_SetMachineId(anviz\_handle, dev\_idx,MachineId);

### 2.83.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

## 2.84 CChex\_ManageLogRecord

### 2.84.1 Function

【Function】Setting device Communication device ID

### 2.84.2 Request

【Mode】int CChex\_ManageLogRecord(IntPtr CchexHandle, int DevIdx, ref CCHEX\_MANAGE\_LOG\_RECORD Param);

【Parameter】CchexHandle：successfully create the handle，Input[Parameter]；

DevIdx: Index of device，Input[Parameter]；

Param： //

Byte[4] start\_date; // The second since of after 2000 years, 2000.1.2

Byte[4] end\_date; //The second since of after 2000 years, 2000.1.2

Byte CmdType; //Extended command ：　0x00 Get the total number of current time periods

0x01 Download the current time period log record

0x02 delete all records in the current time period

0x03 Set real-time report log record

0x04 Get the status of real-time reporting records

Byte AutoFlag; //0:Close real-time report log record 1: Enable real-time report log record

### 2.84.3 Respond

【Return value】1：The command was executed successfully；Minus：Execute command failure

【Actual Data】CChex\_Update Type Return CCHEX\_RET\_MANAGE\_LOG\_RECORD\_TYPE //90

Data Part：

uint MachineId; // Device ID

uint CmdType; // Extended command

0x00 :Result judge success,TotalNum is Total number of the log

0x02 :Result is valid Delete success or not

0x03 Set real-time report log record

0x04 Get the status of real-time reporting records

0x05 Real-time reporting record

Int Result; // 0:Succes -1：Failure

uint IsAuto; // Auto-tagging

uint TotalNum; // Total number of the log

CmdType == 0x00:Result==0 Total number of the log

CmdType == 0x01:Result==0 Total download number of the log

uint CurNum; // The log id of the current logByte[5] EmployeeId; //Employee Id

Byte[4] Date; //Event date The second since of after 2000 years, 2000.1.2

Byte[2] LogType; //Log Type 0x0001 open door 0x0002 close door

0x0003 door sensor 0x0004 Tamper alarm

0x0005 Exit button 0x0006 burst open the door

Byte[2] LogLen; //Log content length

Byte[3] padding; //Fill alignment invalid data

### 2.84.4 Sample

int ret = CChex\_ManageLogRecord(anviz\_handle, dev\_idx,ref Param);

### 2.84.5 Notice

1. Make sure that CChex\_Start has been started successfully before run.

# Return value

1：Success；

-1：Parameter Error；

-2：Lack of device resources；

-3：Unknown Error；